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Note: Refer to key numbers on relevant Porphyrios and Hopkins planning drawings for location of external envelope materials and finishes







	1.0 - Student Residences – Blocks J2, J3, J4, J5 and Building 11


	Location
	Description

	Image

	External Masonry Walls – Blocks J3, J4, J5 and Building 11

( Drg. Key Ref: 1 )
	Half brick clay facing brickwork in stretcher bond with bucket handle or recessed pointing from the following range
· Orange/Red: Ibstock 'Red Stock' Ref 4930
· Brown/Red: Ibstock 'Himley Worcestershire Mixture' Ref 0317
· Yellow: Ibstock 'Ivanhoe Cream' Ref 0054
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	External masonry walls– Blocks J2

(Drg. Key Ref: 1 )
	Half brick clay facing brickwork in stretcher bond with bucket handle or recessed pointing 
· Red : Ibstock ‘Heritage Red Blend’ reference 4986
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	Brick flat arches to windows

( Drg. Key Ref: 2 )
	Prefabricated flat brick radial arches to window heads with brickwork to match surround masonry walls







	[image: C:\Documents and Settings\paul.mckee\Local Settings\Temporary Internet Files\Content.Word\Brick arch.jpg]

	Reconstituted stone rusticated base, string courses and parapet copings

( Drg. Key Refs: 3,4,6 )
	Wet cast reconstituted stone rusticated concrete panels to ground and first floor levels, feature string courses and parapet copings with a high grade aggregate lightly acid etched finish to all visible faces





	
[image: C:\Documents and Settings\paul.mckee\Local Settings\Temporary Internet Files\Content.Word\rusticated base.jpg]






	





















	Reconstituted stone porches to entrance doors, feature window surrounds and balconies

( Drg. Key Refs: 8,9 )
	Wet cast reconstituted stone concrete entrance porches and feature surrounds with a high grade aggregate lightly acid etched finish to all visible faces
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	Reconstituted stone cills

( Drg. Key Ref: 5 )
	Wet cast reconstituted stone concrete cills with a high grade aggregate lightly acid etched finish to all visible faces
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	Powder coated aluminium casement windows

(Drg. Key Ref: 14 )
	Technal polyester powder coated thermally broken aluminium casement window frames, mullions and transoms complete with factory sealed green or grey antisun double glazed units.



	
[image: ]



	













[image: FXi46]











	2.0 - Manufacturing Facility


	Location

	Description
	Image

	External masonry piers

(Drg. Key Ref: 1 )
	Half brick clay facing brickwork piers in stretcher bond with bucket handle or recessed pointing 
· Red : Ibstock ‘Cheddar Red’ reference 0610
	

[image: C:\Documents and Settings\paul.mckee\My Documents\2012 PROJECTS\022312 - Swansea University\Planning Finishes Schedule\Bricks\cheddar-red-2.jpg]

	





















	Metal cladding

(Drg. Key Ref: 5 )
	Vertically fixed Eurobond Europanel flat composite panels with integral window adaptor and powder coated horizontal feature channels at floor and eaves levels
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	Fabric roof structure to internal street

(Drg. Key Ref: 27 )
	Translucent fabric covering on powder coated tubular steel tapered trellis roof structure with marine grade stainless steel cables and concealed stainless steel bolts
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	Powder coated aluminium windows and shading louvres

(Drg. Key Refs: 7,10 )
	Technal polyester powder coated thermally broken aluminium window system with side and top hung opening lights complete with factory sealed green or grey antisun double glazed units, insulated spandrel panels and powder coated vertical solar shading louvres.
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	Glass blocks

(Drg. Key Ref: 28 )
	190x190x80 clear glass blocks set in steel channel support framework with 10mm white mortar joints to fire escape stairs





	[image: http://www.sevesglassblock.com/usr/foto/catalogo/big/udine_2.jpg]




























	Service yard goods and personnel access doors

(Drg. Key Ref: 23 )
	Stokvis or similar insulated vertical lift goods doors with 2nr. vision panels. Steel powder coated insulated personnel access and fire escape doors.
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	Roof level plant enclosures

(Drg.Key Ref: 8 )
	Polyester powder coated ventilation louvers or matching profiled metal cladding to roof level plant enclosures.





	[image: http://www.stertiluk.com/stertilstokvis/images/stratafullylouvred-pic1.jpg]
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	3.0 - SMaRT Building


	Location

	Description
	Image

	External masonry piers

(Drg. Key Ref: 1 )
	Half brick clay facing brickwork piers in stretcher bond with bucket handle or recessed pointing 
· Red : Ibstock ‘Cheddar Red’ reference 0610
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	Low level metal cladding panels including transformer compound

(Drg. Key Ref: 5 )
	Vertically fixed Eurobond Europanel flat composite panels with integral powder coated window adaptor 
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	High level trapezoidal metal cladding

(Drg. Key Ref: 6 )
	Horizontally laid trapezoidal CA32 1000W profile finished in colourcoat HPS 200 
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	Powder coated aluminium windows and solar shading louvres

(Drg. Key Refs: 7,9 )
	Technal polyester powder coated thermally broken aluminium window system with side and top hung opening lights complete with factory sealed green or grey antisun double glazed units, insulated spandrel panels and powder coated horizontal solar shading louvres.
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	Main entrance screen and doors 

(Drg. Key Ref: 13 )
	Powder coated aluminium curtain walling with power assisted doors and factory sealed green or grey antisun double glazed units
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	Roof level plant enclosures

(Drg. Key Ref: 8 )
	Polyester powder coated ventilation louvers or matching profiled metal cladding to roof level plant enclosures.
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	4.0 - Business and Economics Building


	Location

	Description
	Image

	External masonry walls

(Drg. Key Ref: 1 )
	Half brick clay facing brickwork piers in stretcher bond with bucket handle or recessed pointing 
· Red : Ibstock ‘Heritage Red Blend’ reference 4986






	
[image: Heritage Red Blend]

























	Precast concrete fair faced columns, beams and copings

(Drg. Key Refs: 2,3,4 )
	Wet cast precast concrete columns and beams to ground floor levels and parapet copings with a high grade aggregate lightly acid etched finish to all visible faces





	
[image: Chethams School of Music]





	






















	Metal cladding panels to ground and third floors

(Drg. Key Ref: 5 )
	Vertically fixed Eurobond Europanel flat composite panels with integral powder coated window adaptor 
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	Powder coated aluminium windows and solar shading louvres

(Drg. Key Refs: 7,10 )
	Technal polyester powder coated thermally broken aluminium window system with side and top hung opening lights complete with factory sealed green or grey antisun double glazed units, insulated spandrel panels and powder coated horizontal solar shading louvres.
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	Main entrance curtain walling and solar shading louvers

( Drg. Key Refs: 7,20 )
	Powder coated aluminium curtain walling and vertical solar shading louvers with power assisted doors and factory sealed green or grey antisun double glazed units
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	Roof level plant enclosures

( Drg. Key Ref: 8 )
	Polyester powder coated ventilation louvers or matching profiled metal cladding to roof level plant enclosure.
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	5.0 - Learning and Resource Building


	Location
	Description

	Image

	External Masonry Walls

(Drg. Key Ref: 1 )
	Half brick clay facing brickwork in stretcher bond with bucket handle or recessed pointing from the following range
· Orange/Red: Ibstock 'Red Stock' Ref 4930
· Brown/Red: Ibstock 'Himley Worcestershire Mixture' Ref 0317
· Yellow: Ibstock 'Ivanhoe Cream' Ref 0054
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	Reconstituted stone rusticated base, window surrounds and parapet copings

(Drg. Key Refs: 3,6,8 )
	Wet cast reconstituted stone rusticated concrete panels to ground floor level, window surrounds and parapet copings with a high grade aggregate lightly acid etched finish to all visible faces
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	Reconstituted stone wall panels

(Drg. Key Ref: 5 )
	Wet cast reconstituted stone concrete wall panels with a high grade aggregate lightly acid etched finish to all visible faces





	[image: C:\Documents and Settings\paul.mckee\Local Settings\Temporary Internet Files\Content.Word\imgCAYHZV8B.JPG]





	

























	Powder coated aluminium windows 

(Drg. Key Ref: 12 )
	Technal polyester powder coated thermally broken aluminium window system with top hung opening lights complete with factory sealed green or grey antisun double glazed units
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	Main entrance curtain walling and collonettes

(Drg. Key Ref: 16 )
	Powder coated aluminium curtain walling and vertical feature collonettes with power assisted doors and factory sealed green or grey antisun double glazed units
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	Roof level plant enclosures

(Drg. Key Ref: 18 )
	Polyester powder coated ventilation louvers or matching profiled metal cladding to roof level plant enclosures.









	[image: http://www.stertiluk.com/stertilstokvis/images/stratafullylouvred-pic1.jpg]







	



[image: http://www.archprof.co.uk/walls/louvre/profile.jpg]














	6.0 - Great Hall


	Location

	Description
	Image

	Reconstituted stone wall panels

( Drg. Key Ref: 31 )
	Wet cast reconstituted stone concrete wall panels rusticated to base course with profiled detailing to parapets, pediments etc., in a high grade aggregate lightly acid etched finish to all visible faces






	[image: North Kent Police Station]
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	Powder coated aluminium windows 

( Drg. Key Ref: 32 )
	Technal polyester powder coated thermally broken aluminium window system with top hung opening lights complete with factory sealed green or grey antisun double glazed units
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	Main entrance curtain walling and collonettes

(Drg. Key Ref: 33,34)
	Powder coated aluminium curtain walling and vertical feature collonettes with power assisted doors and factory sealed green or grey antisun double glazed units







	[image: C:\Documents and Settings\paul.mckee\Local Settings\Temporary Internet Files\Content.Word\Thorp Brindley Place.jpg]








	





















	Main roof

(Drg. Key Ref: 30 )




	Kalzip or similar stucco embossed natural finish aluminium built up standing seam roof system







	[image: http://www.euroclad.com/media/3229/soundwell%20college.jpg]
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