8 WIND STREET NEATH
APPLICATION REF: - P2019/5217
LA PLANNING CONSENT 
CONDITION 7:-
“CONDITION 7: -
No development shall take place until details of both hard and soft landscape works have been submitted to and approved in writing by the Local Planning Authority.
These details shall include:
a) Statement setting out the design objectives and how these will be delivered;
b) Existing and proposed levels.
c) Means of enclosure and retaining structure;
d) Other vehicle and pedestrian access and circulation areas;
e) Hard surfacing materials (including samples);
f) Minor artefacts and structures (e.g. furniture, refuse store, signs, etc.).
Soft landscape works shall include; planting plant written specifications (including cultivation and other operations associated with plant and grass establishment); schedules of plants noting species, plant supply sizes and proposed numbers / densities where appropriate; an implementation programme 9including phasing of work where relevant).
The landscaping works shall be carried out in accordance with the approved details during the first planting season immediately following completion of the development and retained as such thereafter.
RESPONSE:-	
a)  The design objective is to provide a compact and attractive but simple arrangement providing a limited amount of on-site parking, surface finishes intended are by using a combination of Brindle paviours to paving areas and tarmac to parking road areas. 
Due to the location landscaping potential is restricted and it is currently envisaged that it will be provided by bespoke planting tubs.
b) The site is relatively flat with the rear garden approx. 10.76, the floor levels to the building are approximately 150mm above this, all existing levels will be are maintained and remain as they are currently. 
c) The rear space is enclosed on two sides by the existing structures of Supadrug and Boots, the rear yard is approached via Boots service yard and it is the intention the rear yard will be fenced in across this elevation with PPC hoop top fence and gates as shown on drawing A1103 -6 rev D.
d) The pedestrian entrance to the front will be by the existing steps and ramp on Wind Street with a further disabled entrance to the rear from the proposed car parking area and yard to the rear.
e) Brindle paviours (data sheet attached) and tarmac roads to join to existing in rear service yard.
f) [bookmark: _GoBack]n/a
