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           [image: image1.png]Staying COVID-19 Secure in 2020

We confirm we have complied with the government's
guidance on managing the risk of COVID-19

o FIVE STEPS TO SAFER
WORKING TOGETHER

We have carried out a COVID-19 risk assessment and
shared the resuts with the people who work here.

We have cleaning, handwashing and hygiene procedures.
inline with guidance.

We have taken allreasonable steps to help people work
from home.

We have taken allreasonable steps to maintain a 2m
distance in the workplace

Where people cannot be 2m apart, we have done everything
practical to manage transmission risk

Q 0 0 00

Andrew Murphy Sth July 2020

Employer Date

Moorgate Consulting. (07964 106 382)
all: ¢onsulting @moorgate: london.com)





                         L. G. Murphy (Swansea) Limited

                                                        METHOD STATEMENT

              Construction (Design and Management) Regulations 2015 
For the purpose of this method statement the Client is the organisation L. G. Murphy (Swansea) Ltd are contracted to.
_____________________________________________________________________________________________
Client:/Principal Contractor :  Sterling Construction  Ltd                      Principal Designer: 
                                    .                                                                                                                                                                         
 Contact::  TBA                                                                                              Contact  TBA
Demolition Contractor: LG. Murphy (Swansea) Limited                       Structural Engineer: 
                                        11, Prospect Park                                                              
                                         Queensway                                                          Contact   TBA                          
                                         Swansea West Industrial Estate                                        
                                         Fforesfach Swansea SA5 4ED                                                                                                                                                                          
Contact: Andrew Murphy                                                                                                  
Telephone: 07774730276                                                      
 E-mail: andrew.lgmurphy@btconnect.com                                                                                                                                                
_____________________________________________________________________________________________

Site Location: 26 Alfred Street, Neath
________________________________________________________________________________________
Description of Works: Carry out  demolition works in accordance with  the Client’s scope of works.     

 ________________________________________________________________________________________
L. G. Murphy (Swansea) Limited Site Supervision: -
Mr Andrew Murphy –Project /Site Manager – Responsible for overall management of the entire Project.

Geraint Williams- Contracts Manager– Reporting to the Project Manager
Number of employees involved: - 1 Site Supervisor, 3 operatives
Contact telephone numbers/e-mail addresses: - 
Andrew Murphy: 07774730276 E-mail: andrew.lgmurphy@btconnect.com
Geraint Williams: 07968 750232 E-mail: geraint.williams@live.com
Safety Adviser: Moorgate Consulting: 07964106382. E-mail:consulting@moorgate-london.com
 __________________________________________________________________________________________
Information  supplied by Client – Demolition Asbestos Survey by Excal Ltd, March 2020. – Report No. 286-01-01.R1
____________________________________________________________________________________________
SITE SECURITY 
Site secured byHeras fencing/hoarding by Principal Contractor . Gates secured . Plant and vehicles locked out of hours.
___________________________________________________________________________________________
SITE ACCESS

Banksman control in place as necessary.
________________________________________________________________________________________
DESIGN /SITE HAZARDS 
Presence of Asbestos Materials. 
Working at Height

Plant 
 The Wildlife and Countryside Act 1981 (WCA)
  European Union Council Directive 92/43/EEC of 21 May 1992 on the Conservation of Natural Habitats and of Wild Fauna and Flora.
 Conservation of  Habitats and Species Regulations (2010).
 A  lack of  trees in the area would imply there are no bats on site, however,  if bats do exist on the site a Derogation Licence  must be issued 
 to the Client by an Ecologist to allow demolition to proceed.
_____________________________________________________________________________________
METHODS OF EXECUTION

                               EQUIPMENT                                                                   TASK
ACCESS
	ACCESS EQUIPMENT
	
	        PLACE TO BE USED


                           Full height scaffold                                                 On building for part Demolition
                           Podiums/ towers                                                       Soft stripping 
____________________________________________________________________________________
MATERIALS STORAGE

Recovered materials will be temporarily stored on hard standing. They will always be stored so that they do not present a hazard to anyone else in the vicinity.  Considerations, which will be applied when using a designated storage area will be: -
(a) Preventing falls of materials

(b) Minimising trips and collisions

(c) Blocking safe access and egress routes

(d) Flammability of materials to be stored
____________________________________________________________________________________________

ELECTRICAL
Any  electrical equipment used on this project will be of 110v supply or battery operated and PAT tested. Visual checks of the equipment will be undertaken before each use.

_____________________________________________________________________________________________
  PLANT

All plant to be used will be serviced and maintained in accordance with the manufacture's guidance and any statutory instructions.  On this project the following plant will be utilised: -

	PLANT
	
	USE


8-14t   360° Excavator                                                                            Demolition/Waste handlng
16/20  yard waste skips                                                                                 Waste removal 
_____________________________________________________________________________________________
MATERIALS AND SUBSTANCES
All workers will be given information and/or instruction on the materials and substances to be used or found to be present on this project.  This information will be extracted from the safety data sheets and COSHH assessments.  This information will be given in the pre-work briefing mentioned below under the heading “Training”.  

Other than the materials and substances listed below, no other substances will be brought onto site without the client’s permission. List of materials and substances to be used: -
	MATERIAL/SUBSTANCE
	
	USE


                                 Diesel Fuel                                                                               Plant fuel

__________________________________________________________________________________________
TRAINING

All workers will only be allowed to undertake work that they have been suitably instructed and trained to carry out. Where statutory training is required this will have been undertaken prior to commencing work.  Copies of statutory training certificates are available on request. Supervisors, Managers and operatives hold appropriate current CSCS and CPCS cards. 
L.G. Murphy are members of the National Demolition Training Group (NDTG ) who provide regular training to the Company
Pre-work briefings will take place with all workers prior to commencing work.  The briefing will include the following: -
· This document

· Safety Data sheets and COSHH Assessments 

· Work Sequences as per work programme.

· Safe Working Arrangements 

· Risk Assessments (enclosed)

· Any information supplied by the Client e.g. Site Rules.
____________________________________________________________________________________________                                                                                                                                                                                                            
PERSONAL PROTECTIVE EQUIPMENT (PPE)
Where PPE is identified as necessary for any part of the work, the PPE will have been assessed for its suitability prior to it being used.  All workers will receive instruction at the pre-work briefing on the use, storage and maintenance of any PPE to be used.  The wearing of PPE will be enforced using our disciplinary procedure.
The following is a list of PPE conforming to BSi/EN specifications and standards intended for use on this project: -
	PPE
	
	USE


Hard Hats                                                                       Head protection

Gloves                                                                            Hand protection


Hi Visibility vests                                                             Alert other workers

Safety footwear                                                               Foot protection

Ear protection                                                                  Hearing protection

Eye Protection                                                                 Eye protection

FFP3  or  Face Fit Respirator (Asbestos dust 
filter toEN14387:2004 -F EN143:200 -Filter performance)                              Respirable dust /Covid-19 protection                                       
Full body safety Harness with secured safety line          Work at height
Disposable Overalls                                                        Protection from dust.
_____________________________________________________________________________________________
WELFARE AND FIRST AID

Welfare and Toilet facilities will be provided by the PC  on the site These all conform to the requirements of the Construction (Design and Management) Regulations 2015 – Regulations 4(2)(b),13(4)(c) and 15(11). 

A First Aid kit will be available at site along with an emergency eye wash kit. 
First Aid arrangement to include Covid-19 precautions for administration of First Aid for example to an unconcitious person!
___________________________________________________________________________________________
SEQUENCE OF WORK                                    
If at any time the sequence of work has to be changed this will not be done without first consulting with the PC : Sterling Construction Ltd
Visit to site and survey by L.G. Murphy (Swansea) Limited to familiarise themselves with the site including the structural condition/design of the buildings and  to determine safe sequence of work for the preparation of Method Statement and Risk Assessments. Site meeting held with Client  / PC to discuss project.
Welfare facilities put in place  by thec Principal Contractor conforming to the Construction (Design and Management) Regulations 2015 – Regulations 4(2)(b),13(4)(c) and 15(11). 
Written confirmation of erlectrical disconnection/isolation to be provided to L.G. Murphy (Swansea) Limited.

Induction Briefings provided to all operatives and sub-contractors personnel to include Method Statements and Risk Assessments, , supervision and communications, location of pedestrian designated safe routes, identification of  retricted areas,  welfare and first aid facilities, site rules, emergency evacuation routes, fire precautions and waste management and environmental arrangements.
 Site Induction provided by the Principal Contractor
            Sequence of Work :

· Set exclusion zone using hazard tape /barriers and signage under control of Banksman
· Ensure all services are disconnected to building – Isolation Certs available prior to any Demolition Works.

· Building checked clear of personnel. Entrances secured to prevent entry.
· Asbestos removal and disposal carried out .Clearance Certificate to be provided prior to start of demolition works.
· Soft stripping works to interior of building. Waste placed in bins for disposal .
· Full height scaffolding erected  to external elevations of building.
· Working in exclusion zone operatives wearing  safety harness with secured safety lines, working off 
         scaffolding using hand tools, remove roof and reduce part walls in a controlled and progressive manner ensuring stability throughout.
· General waste segregated and placed in bins for disposal off site to a licenced recycling facility.
· With walls reduced to safe height, using appropriate 360 deg excavator with selector grab working under banksman control to reduce the remaining internal and external walls of the building to slab level in a controlled and progressive manner ensuring stability throughout.. Use water spray to suppress dust evolution.

· Using  excavator with grab attachment places waste masonry material in designated area  and 
        separates and places all other waste into designated  waste bins for removal from site..                                                                                                                                                                                                          
· All masonry  - Concrete/ brick etc removed off site in 6/8 wheeler lorries.

Slab , Footings Removal
· Re set exclusion  zone using hazard tape/ barriers and signage under control of banksman.
· Excavation permit to excavate issued by Principal Contractor and any controls required put in place.

· Working in exclusion zone under control of banksman , use 360deg excavator  - with HD Breaker if required - to remove slabs and footings. Material hauled off site.

Signed: …………………………………………Date:
                               Andrew Murphy, Managing Director
Employee Agreement.
“The contents of this Method Statement and attached Risk Assessments have been explained to my satisfaction and are fully understood.

 I understand that I must adhere strictly to the sequence of operations and all other instructions above and that in the event of any need to deviate from the methods laid down I must stop until agreement is reached and recorded in writing on any revised method of work.”
Signxbelow: Signatures waived due to Covid-19. Verbal confirmation of understanding only required from operatives!
WAH Operations.  Emergency Plans
WAH Operations – Harness Suspension. 

Health Consequences of Suspension 
All users of personal fall protection systems and others involved with work at height should be aware of the following precautions that might need to be taken in the event of a casualty being in a suspended position. 

· The longer the casualty is suspended without moving, the greater the chances are of serious consequences developing. Therefore, an injured person hanging in a harness awaiting rescue should be removed from upright suspension as quickly as possible. The aim should be to do this within 5 minutes. This is particularly important for a casualty who is a motionless 

· A conscious casualty should be encouraged to exercise their legs gently, to stimulate circulation of blood. 

· Regarding position of the casualty: 

· During rescue, a position with the lower limbs slightly elevated may be preferable. 

· If suspension has occurred alert medical services immediately. 

· Following an accident, the casualty should be: 

· Removed from the suspended position to the nearest point of safety. 

·   Assessed by a qualified first aider. 

· Given professional medical assistance as quickly as possible. 

Users of personal fall protection equipment should be aware of potential complications which can occur from prolonged suspension. Whilst speed is essential it is vital that the specially trained rescue team wear full body harness and secured fall restraint before commencing any rescue operation.

	                                       If someone is suspended in a harness

                                            React Immediately

                You only have a short time to rescue them especially if they are unconscious

   If it is unlikely that site rescue team will be able to affect a rescue within 5

   minutes the Fire & Rescue and Ambulance Services should be called

   immediately on 999

 


Training    

It is crucial that rescue teams are exercised regularly in the techniques required to quickly perform rescue operations including familiarity with rescue equipment which is available at site. 

______________________________________________________________________________________________________

References:  

The Work at Height Regulations 2005

International Powered Access Federation. Guidance on Emergency Rescue.

BS 8454: 2006. Code of practice for the delivery of training and education for work at height and rescue                                                

HSE - General Information
                       L. G. MURPHY (SWANSEA) LIMITED
                       
MANUAL HANDLING RISK ASSESSMENT 

            MANUAL HANDLING OPERATIONS REGULATIONS, 1992, as amended  2002

	SECTION 1

	Description: Operatives carry out demolition by hand



	Reference: 
	
	Date: TBA
	

	Assessor: 

	

	Location:  26  Alfred Street, Neath
	

	Number  involved in the task: 3
	Level of experience: High


	Overall assessment of the risk of injury: Low with controls in place including supervision. 
	
	
	
	


	SECTION 2

	Remedial Actions:

	Manual handling limited to materials weighing less than 25kg per man 

	Limited to short term occasional lifts by trained experienced operatives.

	Mechanical aids utilised wherever practicable  24 ton Excavator. Wearing of PPE provided enforced under Site Rules.

	Risk Assessments, Method Statements and Training provided.

	Direct supervision by experienced Management in place throughout.

	

	

	

	

	Demolition by Hand- 

	Manul handling limited per man to 3 bricks or equivalent each weighing 3.5 kg including attached cement mortar/render. Total weight per lift 10.5 kg

	

	

	

	

	

	


	
                L.G. Murphy (Swansea) Limited   
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                          Swansea West Industrial Estate

                                      Fforestfach,                                                                                  

                               Swansea, SA5 4ED   


	        Health & Safety Policy Forms
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L. G. MURPHY (SWANSEA) LIMITED

                              MANUAL HANDLING RISK ASSESSMENT

                        MANUAL HANDLING OPERATIONS REGULATIONS, 1992, as amended  2002
	SECTION 3

	Considerations
	If yes, tick appropriate level

of risk
	Risks arising from the task
	Remedial action

	
	
	
	

	
	Low
	Med
	High
	
	

	The tasks - do they involve?
	
	
	
	
	

	Holding loads away from the trunk
	
	
	
	
	

	Twisting
	
	
	
	
	

	Stooping
	
	√
	
	Strain when lifting material
	Training and correct lifting techniques employed

	Reaching upwards
	
	√
	
	Strain when lifting material
	Training and correct lifting techniques employed

	Large vertical movement
	
	
	
	
	

	Long carrying distances
	√
	
	
	Strain when carrying
	Material dropped inside building DZ

	Strenuous pushing / pulling
	
	
	
	
	

	Repetitive handling
	
	
	
	
	

	Insufficient rest or recovery
	
	
	
	
	

	Work rate imposed by a process
	
	
	
	
	

	The loads - are they?:
	
	
	
	
	

	Heavy
	
	√
	
	Strain when moving material
	24 to n Excavator,

	Bulky / Unwieldy
	
	√
	
	Strain when moving material
	24 ton Excavator 

	Difficult to grasp
	
	
	
	
	

	Unstable / Unpredictable
	
	
	
	
	

	Intrinsically harmful(e.g. sharp / hot)
	
	
	√
	Cuts from handling material
	Appropriate PPE provided.

	The working environment - are there?:
	
	
	
	
	

	Constraints on posture
	
	
	
	
	

	Poor floors
	
	
	
	
	

	Variations in floor levels
	
	
	
	
	

	Hot/cold/humid conditions
	
	
	
	
	

	Strong air movements
	
	
	
	
	

	Poor lighting conditions
	
	
	
	
	

	Individual capability - does the job?:
	
	
	
	
	

	Require unusual capability
	
	
	
	
	

	Hazard those with a health problem
	
	
	√
	Harm to individual
	Only employees in good health employed on this task.

	Hazard those who are pregnant
	
	
	√
	Harm to mother/child
	Pregnant employees not employed on this task.

	Call for special information / training
	
	
	√
	Harm to individual
	Demolition RA and Method Statement. Demolition Phase H & S Plan and MH training. Induction training.

	Other factors
	
	
	
	
	

	Is movement or posture hindered by clothing or personal protective equipment?
	YES
	NO
	
	

	
	
	√
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                          L. G. MURPHY (SWANSEA) LIMITED

                                           C.O.S.H.H. ASSESSMENT
                  Control of Substances Hazardous to Health Regulations 2002 as amended 
	SUBSTANCE :

Diesel Fuel – Ultra Low Sulphur Derv
	ID – 26 Alfred Street, Neath

	DESCRIPTION OF USE:

As a gas oil fuel for plant and on-road vehicles.



	LIKELIHOOD
	Possible
	
	
	

	SEVERITY
	Major
	
	
	

	EXPOSURE
	Short Term
	
	
	

	QUALIFIED RISK RATING 
	High - without Controls in place.

Low – with Controls in place.                          

	PERSONS AT RISK
	ROUTES OF ENTRY
	                            HAZARDS

	Operator √

Other Employee √

Contractor√

Visitors√
Young Persons

Expectant Mother


	Inhalation √

Ingestion  √

Absorption √

Injection√ See Note 2.

	Corrosive                             Other / Specify-See Note1 below
Toxic                                    Asphyxiant

Flammable√ Flash Point 60°  Harmful √

Highly Flammable                Extremely Flammable

Explosive                              Irritant √

Sensitiser √

Note1: May contain Polycrylic aromatic hydrocarbons(PCAs) potential to cause skin cancer (category 3 carcinogen).

Note 2: Injection under skin may have serious medical effects

	Chemical Occupational Exposure Limits, (If applicable).

	CHEMICAL NAME
	STEL
	LTEL

	Complex mixtures of distillate hydrocarbons mainly paraffinic, napthenic and aromatic in range C10-C28 with additives. 

Note.  Additives do not contribute any additional hazard.
	10mg/m³ (15 minute ref)
	5 mg/m³

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	CONTROLS: 

Transfer of fuel to vehicles pumped by electric pump through hose with trigger nozzle from purpose designed bunded fuel bowser ort Transcube
Smoking is not permitted on site. No consumption of food or drink permitted in the workplace.

Well-ventilated area. Nitrile gloves, goggles (none venting), boots, disposable overalls with hood worn by operator. 

Strict hygiene followed including washing facilities Access to area strictly restricted.
Training provided to all operatives.

	Does the substance require a DSEAR assessment?             
	Yes 
	
	
	

	Are there any restrictions allocated to this substance?          
	Yes
	
	
	

	If “YES” please specify: Dispose of as hazardous waste

                                       Harmful to the environment.

                                           Transport Classification: UN Flammable Liquid. Class 3 (111)

                                       Avoid flames. Flash Point 60°C min

	RECOMMENDATIONS / REMEDIAL ACTIONS: Ensure movement onto and off site controlled by banksman.
Maintain existing controls. Monitor and review every 12 months

Provide spill kit.


                                                                                                                              L. G. Murphy (Swansea) Limited            

                                           Risk Assessment – Construction Design and Management Regulations 2015 
   Project Location:    26 Alfred Street, Neath
  Project: : Carry out  demolition works in accordance with  the Client’s scope of works.     
   Client:  Sterling Construction Ltd
	No
	      Hazards 


	Risks Arising


	Persons at Risk
	Level of  Risk

 with Existing

    Controls
	  [image: image2.png]Frequency




	                       Additional Control Measures
	      Risk

 Assessment With Controls

	
	
	
	
	L
	S
	R
	
	
	L
	S
	R

	1
	Hazardous       Substances- Covid -19
	Fatality/ ill health due to exposure to

Covid-19 vrus
	LGM Staff and their families

Others


	5
	5
	25
	High
	Covid -19 Government advices to employers put in place including 2m work distancing, Hot water hand washing facilities, and hand sanitizer made available. Staggered breaks, Travel to and from work by individuals in own vehicles – No sharing of transport permitted. Face coverings/face masks, overalls   and eye protection available as required. Signatures waived due to Covid-19. Verbal confirmation of  understanding  of document such as Rams only required from operatives!
	2
	5
	10

	2
	Hazardous       Substances- Covid -19
	Fatality/ ill health due to exposure to

Covid-19 vrus
	LGM Staff and their families

Others


	5
	5
	25
	High
	Employees who are at high risk due to under lying health symptoms required to self-isolate and not attend site. An employee or a family member sharing the same house who displays a dry cough and high fever is required to self-isolate and the employee not attend site. Telephone 111 for advice. Inform Andrew Murphy immediately. 
	2
	5
	10

	3
	Employees 
	Fatality/ ill health due to exposure to hazards
	LGM Staff


	4
	5
	20
	High
	Personnel must have suitable H&S training including holding current CSCS cards. Site induction/site familiarisation carried out by Principal Contractor before starting work. 

Competence and training records to be verified before starting work

Personnel sthat they have read and understand  RAMS- 

	  2
	5
	10

	4
	Hazardous       Substances

	Fatality/ ill health due to exposure to hazardous substances. 
	LGM  Staff


	4
	5
	20
	Low
	Compliance with COSHH Regulations- Information and MSDS provided and assessments carried out where necessary. Welfare facilities provided including washing facilities. Good personal hygiene practices adopted and PPE used. Certificated Training provided. Possible existence of needles on site- precautions taken.

	2
	5
	10


	LIKELIHOOD (L)

5=Very Likely
4=Likely
3=Possible
2=Unlikely But Conceivable
1=Highly Unlikely
	SEVERITY (S)

5=Fatal
4=Major Injury

3= Injury, Illness, Serious Damage

2=Minor Injury/Damage

1=Delay/ Prosecution
	           Risk Level=L x S

	RISK

13-25 Unacceptable Significant Risk. Eliminate Activity.

	
	
	
	8-12 Acceptable Risk. Manage Risk and Monitor.

	
	
	Note

Risk Controls Managed/Monitored by Andrew Murphy
	3-7 Low Risk. Manage Risk and Monitor.


	
	
	
	1-2 Negligible Risk. Monitor.


                                                                                                                       L. G. Murphy (Swansea) Limited            

                                         Risk Assessment – Construction Design and Management Regulations 2015 
   Project Location:    26 Alfred Street, Neath
  Project: : Carry out  demolition works in accordance with  the Client’s scope of works.     
   Client:  Sterling Construction Ltd 
	No
	      Hazards 

	Risks Arising


	Persons at Risk
	Level of  Risk
 with Existing
    Controls
	  [image: image3.png]Frequency




	                       Additional Control Measures
	      Risk
 Assessment With Controls

	
	
	
	
	L
	S
	R
	
	
	L
	S
	R

	5
	Hazardous

Substances/
Asbestos
	Fatality/ ill health due to inhalation of asbestos fibres.


	LGM Staff
Clients Staff 

Public

	5

	5

	25


	Low

	Asbestos removal works carried out in accordance with the Control of Asbestos Regulations, 2012. by others. Clearance Certificate provided to LG. Murphy (Swansea) Limited.prior to demolition.
LGM operatives and Supervisors are trained and certificated in Asbestos Awareness training to recognise asbestos material and to take action if any suspicious material is encountered including withdrawal from the area and reporting to Management. Water spray used to suppress dust evolution throughout. 

	2


	5

	10



	6

	Demolition. Stability during demolition.
	Injury/ fatality due to unintended collapse.
	LGM Staff
	4
	5
	20
	High
	Construction design reviewed. Progressive and controlled demolition carried out according to the principles laid down in British Standard BS6187-2011 Code of Practice for Full and Partial Demolition
Trained well supervised operatives. Experienced qualified Demolition

Contractor and Management. 


	2
	  5
	10

	7

	Work at height
	Injury/fatality to due to falls.
	LGM Staff
	5
	5
	25
	Med
	All work at height carried out in accordance with the Work at Height Regulations by trained operatives. Fiul height access scaffolding provided to external elevations . No ccess onto roofs permitted
 
	2
	5
	10

	 8
	Contact with services
	Injury/fatality
	LGM Staff
	5
	5
	25
	Low
	Written confirmation of services disconnection provided to LGM. 

	2
	  5
	10

	9

	Unauthorised access to area
	Injury/fatality 
	   Public


	4
	5
	20
	High
	Site secured by fencing /hoarding and gates. Warning signage in place. Plant/vehicles locked and keys removed out of hours. 
LGM assumes exclusive access to the demolition sites

	2
	5
	10

	10
	Contact with site transport/ plant
	Injury/fatality 
	LGM staff

   Public

  Visitors

	4
	5
	20
	High
	Pedestrian safe routes demarcated. Traffic Management system controlled by Banksmen. High visibility vest worn by operatives/visitors under strict site rules.  Qualified experienced plant operatives and transport drivers. Hazard lights in use throughout.
	2
	5
	10

	11
	Operation of Plant
	Injury/fatality due to ground collapse.

	LGM Staff
	4
	5
	20
	High
	Ground conditions inspected by Andrew Murphy and found to be suitable for heavy plant. 
	2
	5
	110


                                                       L. G. Murphy (Swansea) Limited            

                                     Risk Assessment – Construction Design and Management Regulations 2015 
  Project Location:    26 Alfred Street, Neath
  Project: : Carry out  demolition works in accordance with  the Client’s scope of works.     
   Client: Sterling Construction Ltd
	No
	      Hazards 

	Risks Arising


	Persons at Risk
	   Level of  Risk
   with Existing
      Controls
	  [image: image4.png]Frequency




	                       Additional Control Measures
	      Risk
 Assessment With Controls

	
	
	
	
	L
	S
	R
	
	
	L
	S
	R

	12

	Respiratory Protection
	Injury/fatality due to inhalation of  harmful substances
	LGM Staff
	5
	5
	25
	Med
	Must be selected for the task to be performed and must conform to BSi/EN specifications and standards. 
Worn under strict site rules. Assessed before us to ensure fit for purpose. Maintained, stored & used correctly

Instructions on correct safe use provided to user.


	2
	5
	 10


	13
	Overalls
	Skin contact with harmful substances
	LGM Staff
	5
	3
	15
	High
	Full coverage and correct size and fit

Must be selected for the task to be performed and must conform to BSi/EN specifications and standards. Worn under strict site rules.

Assessed before us to ensure fit for purpose. Maintained, stored & used correctly

Instructions on correct safe use provided to user.


	2
	3
	6

	14

	Foot Protection
	Crushing, impact and puncturing

injuries to feet and slipping.
	LGM Staff
	4
	4
	16
	High
	Must be selected for the task to be performed and must conform to BSi/EN specifications and standards. Worn under strict site rules.

Assessed before us to ensure fit for purpose. Maintained, stored & used correctly

Instructions on correct safe use provided to user.


	2
	4
	8

	15

	Head Protection


	Injuries to head from falling/flying objects and from bumping head
	LGM Staff
	5
	5
	25
	 Med
	Must be selected for the task to be performed and must conform to BSi/EN specifications and standards.

Worn under strict site rules when there is overhead working or if working in restricted head space or confined spaces

Assessed before us to ensure fit for purpose. Maintained, stored & used correctly

Instructions on correct safe use provided to user.


	2
	5
	10



	16
	Impact on neighbours
	Nuisance due to Noise /Dust/Transport

Damage to arty Wall


	Neighbours
	3
	5
	15
	High
	Dust controls in place. Noise limitation fitted to plant. Traffic management system controlled by Banksmen.  Qualified experienced plant operatives and transport drivers. Hazard lights in use throughout. No parking on roads or obstruction of access roads   
                                                    
	    1
	    5
	5

	17

	Use of CP9 demolition hammer
	Respiratory harm  due to dust

HAV
	LGM Staff
	3
	5
	15
	Med
	Open air ventilated are. Respiratory protection worn under strict site rules. Trained operatives. Short trigger times. Monitored by Site Manager. HAV assessments carried out. Records kept


	1
	5
	5


                                                     L. G. Murphy (Swansea) Limited            

                                     Risk Assessment – Construction Design and Management Regulations 2015 
   Project Location:    26 Alfred Street, Neath
  Project: : Carry out  demolition works in accordance with  the Client’s scope of works.     
   Client: Sterling Construction Ltd
	No
	      Hazards 

	Risks Arising


	Persons at Risk
	   Level of  Risk
   with Existing
      Controls
	  [image: image5.png]Frequency




	                       Additional Control Measures
	      Risk
 Assessment With Controls

	
	
	
	
	L
	S
	R
	
	
	L
	S
	R

	18

	Waste Management
	Harm to the Environment.
	LGM Staff

Public

	3
	3
	9
	High
	Mixed Waste removal from site for recycling/disposal in accordance with Waste Duty of Care in Section 34 of the Environmental Protection Act 1990, the Environmental Protection (Duty of Care) Regulations 1991 
	1
	3
	3

	19
	Environmental damage

	Harm to environment due to demolition works

	  LGM Staff

    Public


	4
	3
	12
	High
	Drains/manhole covers protected Sewer Connection sealed where required. Oil spill kit available.  
	2
	3
	6

	20
	Leptospirosis (Weils Disease).
	Fatality/Ill health due to contact with rat urine.
	LGM Staff
	4
	5
	   20
	High
	Welfare facilities include washing arrangements. Good hygiene standards maintained. Training provided.

	2
	5
	10


                                                                                       Signed:………………………………………Date:
                                                                                                        Andrew Murphy Manging Director
Employee Agreement.

“The contents of these Risk Assessments and attached Method Statement have been explained to my satisfaction and are fully understood. I understand that I must adhere strictly to the sequence of 
operations and all other instructions above and that in the event of any need to deviate from these works must stop until agreement is reached and recorded in writing on any revised method of work.

Signx below    Signatures waived due to Covid-19. Verbal confirmation of  understanding only required from 
               operatives!
Demolition Phase Plan Document Copyright © Moorgate Consulting. All Rights Reserved

Copyright, Designs and Patents Act 1988.












