Impacts of Works on Adjacent Highway

From the record photographs, the back of footway level is at the cill level of the window and some 6 courses above FFL. The external ground level around the new extension is therefore in the order of 750mm below the footway level. We have annotated the attached plan extract with the resulting zone of influence for the existing highway, construction within which would be considered highway retaining. 
On that basis it can be concluded that the proposed extension sits outside the zone of influence of the highway.  On that basis the proposals do not therefore represent any issue in respect of highway retention.
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