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ROOF CONSTRUCTION
New roof construction to consist of 150 x 50 Grade C24 rafters at 400mm centres. Provide 225 x 50mm Grade C24 hip timber. Wind bracing shall be provided as detailed in Technical Bulletin Number 1 produced by the Truss Plate Association Ltd., and current Building Regulations. 
Roof covering to be concrete interlocking tile to match existing fixed in accordance with manufacturer’s instructions to 38 x 25mm treated softwood battens on VPU breathable felt to BS 5534. Hip tiles to be smooth faced clay or concrete angular tiles bedded in tinted cement mortar.
Ceiling joists to be 150 x 50mm Grade C24 timbers at 400mm centres with herringbone strutting at 1/3rd and 2/3rd span.
Ceilings to be 12.5mm or 15mm plasterboards to BS 1230 Part 1, screwed to underside of joists with plaster skim finish to provide 30mins fire resistance.
All structural timber to be Grade GS treated with tanlith preservative treatment in accordance with BS 5268 Part 5 (1977).
All carcassing and first fix softwood timbers in roof or in positions exposed to possible dampness are to be pressure impregnated to BS 5268 Part 5 with severity rating high.
All soffits and fascia boards to be uPVC to BS 7619 incorporating a minimum 25mm continuous air vent with insect proof mesh screen, to allow cross ventilation of roof void areas conforming to Approved Document F Part F2.
Roof voids to be insulated with 300mm Rockwool (or similar) glass fibre insulation quilt laid between joists, to achieve a U- Value of 0.15W/m2K. 
Rainwater goods to be uPVC complying with BS 4576 Part 1. Rainwater gutters to be 100mm with 68mm diameter rainwater pipes all clipped and bracketed strictly in accordance with manufacturer’s specification.
Provide Code 4 lead flashing and soakers at abutment of new roof and existing wall. Lead to be dressed over cavity trays built into outer skin of wall.
EXTERNAL WALLS
Cavity walls to be 325mm thick, comprising outerskin of Class A dense concrete block, 125mm cavity with 75mm Kingspan (or similar) rigid insulation batts, with inner skin of 100mm thick Class A dense concrete block. Cavity wall to achieve a minimum U-Value of 0.21 W/m2K.
Wall ties to be stainless steel vertical twist type at 450mm vertical and 600mm horizontal centres, staggered and doubled up at all openings. All ties to be to BS 1243 and fixed in accordance with BS 5628. Cavities to be closed at eaves, cills and jambs with Thermabate (or similar) closers incorporating a DPC. Cavity to be adequately firestopped at eaves level using a suitable non-combustible material such as Rockwool cavity wall batts. Below ground level, cavity to be filled to within 150 of DPC with lean mix concrete to BS 5328.
Provide Hyload DPC by Ruberoid at 150mm above outside ground level and to all vertical and horizontal openings in accordance with BS 743 and CP 121. Lintels over all external openings to be 2 Nr p.c. concrete lintels incorporating a DPC.
Provide structural steel beams as per Structural Calculations.
WALL FINISHES
External block work walls to receive 2 number coats of sand cement render with dash finish to match existing.
Internal block work walls to receive 2 number coats of sand cement render with plaster skim finish.
Provide architectural skirting to BS 1186 Part 3 to client’s choice to all walls. Backs of skirting shall be knotted and primed prior to fixing. All softwood to receive one coat of primer, two coats of undercoat and one coat of gloss finishing paint to BS 5358.
All plastered walls and ceilings to receive one thinned coat and two full coats of vinyl matt emulsion to BS 7719.
FOUNDATIONS
Foundations to be 600 x 300mm concrete strip type, 30N/mm2 strength concrete, with nominal A142 fabric mesh in bottom, to a minimum depth of 750mm below ground level, and below invert level of any adjacent drains. Actual depth of foundations to be determined following examination of the sub-grade site condition. 
FLOORS
Ground floor construction to achieve U-Value of 0.22 W/m2K comprising 65mm thick cement mortar screed on 75mm thick Kingspan (or similar) insulation batts on 1200 gauge Visqueen damp proof membrane on 100mm thick concrete oversite slab to BS 5328 on 150mm thick well compacted Type 1 granular sub base material. Additional layers of fill to be compacted in 225mm layers.
WINDOWS AND DOORS
Windows to be uPVC double glazed unit to BS 6375, incorporating draft proof trickle vents. Window to provide a minimum of 1/10th daylight and 1/20th ventilated opening area of the floor area of the served room. Background ventilation (trickle vents) to be provided having a total area not less than 65,000mm2 as per table 1.2a of Approved Document F1. Opening should be controllable, secure and located so as to avoid undue draughts. 
Security locks to be fitted to windows. Windows to be double glazed with clear sealed units to BS 6262.  Glazing to be low emissivity Pilkington K glass (or similar) with 16-18mm air gap to achieve a U Value of 1.8W/m2K. 
Internal cill level to be agreed with client, but shall be no higher than 1100mm or lower than 800mm. 
External doors to be uPVC fitted complete with all ironmongery. Any glazing below 1500mm to be toughened glass. Door size to comply with requirements of Approved Document M. Glazing to be as for windows and to achieve a minimum U Value of 1.8W/m2K. 
Provide mechanical ventilation of 60 litres/second to the kitchen area or 30 litres/second if incorporated into cooker hood facility. 
STORM WATER DRAINAGE
Downpipes to discharge to uPVC roddable back inlet gulleys. All pipework to be ‘Osma’ 110mm uPVC below ground quality pipes bedded on and encased in granular material to BS 882, laid to fall as specified by manufacturer. Storm water to discharge to soakaway located 5.0m from building.
FOUL WATER DRAINAGE
All foul water to discharge to existing sewer.
WC to discharge to 100mm diameter branch pipe to soil and vent pipe.
Wash hand basin to discharge via 40mm uPVC waste pipe with minimum 75mm deep sealed trap to soil and vent pipe.
Kitchen waste to discharge via 40mm uPVC waste pipe with minimum 75mm deep sealed trap to rodable trapped back inlet gulley.
All waste pipes and fittings to be in accordance with BS 3380 and BS 5255 and installed to BS 5572. All deep sealed traps to be to BS 3943.All waste pipes and fittings to be in accordance with BS 3380 and BS 5255 and installed to BS 5572. All deep sealed traps to be to BS 3943.
All drainage below ground to be 100mm uPVC Osma (or similar) to BS 4660 or BS 5481 laid strictly in accordance with manufacturer’s instructions and Approved Document H of the Building Regulations 2002. Drains to be laid to a minimum fall of 1 in 40 at a minimum depth of 0.6m, bedded on granular material to BS 882.
Where drains pass through walls or foundations provide 2 number 100 x 150 x 450mm concrete lintels over pipe giving a minimum 50mm clearance all around pipe with both sides masked with a rigid sheet material. Any drain passing under a floor or within 1.0m of a building to be encased in 150mm of concrete.
Inspection Chambers (minimum internal size 450 x 450mm) to be either preformed uPVC chambers or 225mm thick engineering brick to BS 3921. Base to be 150mm thick concrete slab, fitted with standard air tight medium duty frame and cover to BS EN 124. Half round channels to be used in chambers with branches discharging into channel at or above the level of the horizontal diameter. Channel and branches should be benched up to at least the top of the outgoing pipe and at a slope of 1 in 12. The benching should be rounded at the channel with a radius of at least 25mm.
SANITARY FITTINGS
Kitchen sink and units to be to client’s specification and in accordance with BS 1195 and BS 4875.
Provide ceramic tile splash backs 300mm high behind sink. Fittings to be properly supported and silicon mastic applied at all edges adjacent to walls.
Hot and cold water distribution pipework to be 15 and 22mm diameter copper pipes fixed to solid backgrounds with clips. Stop taps to be fitted under sink units. All pipework to be installed strictly in accordance with requirements of Dŵr Cymru’s requirements and current legislation to BS 6700.
CENTRAL HEATING
Extend central heating system. All heating works to be carried out strictly in accordance with the requirements of Approved Document J of the Building Regulations 2002.
Provide thermostatic valves to all radiators. System to be installed by a ‘Gas Safe’ registered contractor.
ELECTRICAL INSTALLATION
To be fully in accordance with the Regulations of the I.E.E. (18th Edition), to BS 7671 and undertaken by an approved electrician, registered on a competent persons scheme. Completion certificates to be submitted to Building Control. All power and lighting points to be at locations agreed with client. All sockets and switches to be located at a height between 450 and 1200mm above floor level. Lighting to be energy efficient lights as supplied by Lampholder (ref www.lampholder.co.uk).
EXTERNAL WORKS
Provide concrete paths to perimeter of new building. Make good all disturbed areas.
ALL WORKS TO COMPLY WITH THE CURRENT BUILDING REGULATIONS. 
ALL DIMENSIONS IN MILLIMETRES AND TO BE CHECKED ON SITE PRIOR TO COMMENCEMENT OF WORKS.
