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ROOF CONSTRUCTION
Roof construction to consist of pre-fabricated roof trusses, 30 degree pitch. The trusses shall be designed in accordance with BS 5268 Part 3 and manufactured by a company that is a member of the TRADA Trussed Roofing Quality Assurance Scheme, marked accordingly, and installed in accordance with their recommendations.
Trusses to be fixed using proprietary truss clips. Wind bracing shall be provided as detailed in Technical Bulletin Number 1 produced by the Truss Plate Association Ltd., and current Building Regulations. Calculations of the trusses to be provided by company prior to manufacture and installation. Wall plate to be 100 x 50mm timber, bedded in mortar and secured to inner skin with 30 x 5 x 1200mm galvanised mild steel straps at 1.0m centres.
Roof covering to be concrete interlocking tiles fixed in accordance with manufacturer’s instructions to 38 x 25mm treated softwood battens on VPU breathable felt to BS 5534. Ridge tiles to be terracotta smooth faced clay or concrete angular tiles bedded in tinted cement mortar.
Gable end walls to be supported by horizontal 30 x 5 x 1600mm galvanised restraint straps with 150mm bend fixed over a minimum of 3 trusses at 2.0m centres.
All carcassing and first fix softwood timbers in roof or in positions exposed to possible dampness are to be pressure impregnated to BS 5268 Part 5 with severity rating high.
All soffits and fascia boards to be uPVC to BS 7619 incorporating a minimum 25mm continuous air vent with insect proof mesh screen, to allow cross ventilation of roof void areas conforming to Approved Document F Part F2.
Rainwater goods to be uPVC complying with BS 4576 Part 1. Rainwater gutters to be 100mm with 68mm diameter rainwater pipes all clipped and bracketed strictly in accordance with manufacturer’s specification.
EXTERNAL WALLS
Raise existing blockwork walls by 225mm.
WALL FINISHES
External block work walls to receive 2 number coats of sand cement render with dash finish.
Internal block work walls to have fair face finish.
ALL WORKS TO COMPLY WITH THE BUILDING REGULATIONS (2012).
ALL MEASUREMENTS ARE GIVEN IN MILLIMETERS UNLESS OTHERWISE STATED AND SHOULD BE CHECKED ON SITE PRIOR TO COMMENCEMENT OF WORKS.
