Details to be agreed in association with conditions 4 (replacement culvert), 5 (junction improvements and associated works phasing programme and any related traffic regulation orders), 6 (access arrangements for maintenance of the new culvert inlet and outlet including a new inlet and grill) of application P2011/0486 (Residential development 10 detached dwellings and associated works) granted on 11 December 2019 (Amended / additional highways and drainage information received 11.02.21 and 25.03.21). 
 
For ease, the below table sets out the comments raised by the Council, as per your email dated the 20th of May, against each Condition, and the Applicants response is noted next to this.
 
	Condition No.
	Issue
	LPA Position
	Response

	4
	Replacement Culvert
	Structural calculations and specification for the proposed culvert are required due to its proximity to the road surface to prove it can take the loading of any traffic etc. 
 
	Please find the following documents attached which look to address this comment:
1. Technical Note (produced by the Vale Consultancy);
1. Section 23 Existing Culvert Proposals & Details (dwg no. 10741/506 rev. 04);
1. Section 23 Proposed Headwall & Trash Screen Details (dwg no. 10741/507 rev. 01);
1. Section 278 General Arrangement (dwg no. 10741/S278_770 rev. 04); and
1. Email correspondence between The Vale Consultancy and Marshals confirming culvert length. With regard to the referenced 180m long it’s a typo error in the email from Robin Powell to Jane Woolston (dated 6th July 2020), and should read 18.0m, as the existing culvert is actually 17.3 liners metre and the replacement culvert is 7 m. 

	5
	Junction Improvement
	The junction improvements and tro’s appear acceptable in principle and the submitted phasing indicates that these works are in phase 1. It is however unclear how access will be maintained when they are doing these works. 
 
A Traffic management plan referred to in the submitted documents. This  needs to be provided  in relation to constant access for the nursing home, not just for emergency access but for day to day access, servicing, visitors,  deliveries etc how is this to be maintained, are there temporary arrangements necessary,  and has this arrangement and process been agreed with the owners or other users of the access.  Evidence of this agreement should be provided if this is in place. 
 
It is not for the planning or highway Authority to agree these arrangements. As the nursing home is owned and run by the Authority, who have you been discussing and agreeing this with?
	A Traffic Management Plan (2. IMSF36 Traffic Management Plan) has been prepared by Manning Construction which contains 3-way temporary traffic signal plan prepared by Amberon (drawing ref. SG/10.06.21/S66164).
 
Please also see enclosed documents confirming access arrangements with the nursing home. As can be seen within the attached correspondence, there has been ongoing dialogue between Manning Construction and the nursing home, resulting in an agreement. The following document evidence this:
 
1. Nursing Home Email Correspondence;
 
The following documents were referenced within the above email correspondence:
 
1. Proposed Site Plan;
1. Appendix - Vehicle Access;
1. Letter to Residents;
1. Temporary Closure of Footpath MOANG2 Glynneath; and
1. Temporary Footpath Closure Order.



 

	6
	Maintenance Access for Culvert Inlet and Outlet
	The Condition says notwithstanding the drawing number quoted. This was due to the lack of information on that drawing. 
 
We require a drawing including lay down area for inspection, like a grasscrete area for parking for example, and a technical note for how access to all the above can be provided and maintained without impacting on the free flow or traffic or highway and pedestrian safety. 
 
There also appears to be  discrepancies or concerns over landscaping and proximity of tree planting protection zones to soakaway and we need to ensure that these don’t conflict or maintenance issues arise in future. 
	 Please find the following documents attached which look to address the comments relating to Condition 6:
 
1. Technical Note (produced by the Vale Consultancy);
1. Section 23 Existing Culvert Proposals & Details (dwg no. 10741/506 rev. 04);
1. Section 23 Proposed Headwall & Trash Screen Details (dwg no. 10741/507 rev. 01);
1. Section 278 General Arrangement (dwg no. 10741/S278_770 rev. 04); and
1. Email correspondence between The Vale Consultancy and Marshals confirming culvert length. With regard to the referenced 180m long it’s a typo error in the email from Robin Powell to Jane Woolston (dated 6th July 2020), and should read 18.0m, as the existing culvert is actually 17.3 liners metre and the replacement culvert is 7 m.
 
In addition to the above, a revised landscaping scheme was submitted on the 25th of March 2021 (Landscape Proposals (dwg no. 002 rev. A), this has been attached for ease.
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