	Site Address: Pant Celydd

	Operation:
	Excavations: Buried DCWW Assets
	215 (PC)

	 FORMCHECKBOX 
Check boxes as appropriate

	Hazards identified:

 FORMCHECKBOX 

Contact with underground power cables.

 FORMCHECKBOX 

Rupturing of gas pipes leading to leaks, fire or explosion.

 FORMCHECKBOX 

Rupturing of water pipes causing flooding and damage.

 FORMCHECKBOX 

Cutting of underground telecommunications and interrupting services.

 FORMCHECKBOX 

Rupturing of drains, sewers, culverts etc., and causing health hazards.

 FORMCHECKBOX 

Other

	

	Persons at risk:  FORMCHECKBOX 
Site personnel  FORMCHECKBOX 
General public  FORMCHECKBOX 
Client personnel  FORMCHECKBOX 
 Other

Without controls
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1
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With controls
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3
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If the risk product without controls is high (scoring 6-9), and remains high with controls (scoring 6-9), an alternative safer method of work must be put in place.

	

	Controls considered necessary:

 FORMCHECKBOX 

Work shall be supervised and carried out by competent people, who will be given clear instruction and information.

 FORMCHECKBOX 

Prior to commencement of excavation, all public and local utilities will be requested to provide information of services in the ground of the proposed work area, consult the safety file if applicable.

 FORMCHECKBOX 

A ‘Permit to Dig’ system shall be in position to control works.

 FORMCHECKBOX 

Operatives should look for obvious signs of underground services, e.g. valve covers or patching of the road surface.  Use locators to trace any services. Mark the ground accordingly.  Make sure that the person supervising excavation work has service plans and knows how to use them.  Everyone carrying out the work should know about safe digging practices and emergency procedures.

 FORMCHECKBOX 

After use of locators, trial holes should be carefully dug, using hand tools, to confirm the position of buried services.



	215 Excavations: Buried services - Controls considered necessary (cont.):

 FORMCHECKBOX 

Digging should be carried out alongside the service, rather than directly above it; final exposure of the service should be by horizontal digging. Only spades and shovels should normally be used, but the careful use of picks or forks may be necessary to free lumps of stone or to break up hard layers of chalk or sandstone. 

 FORMCHECKBOX 

Any damage to buried services must be reported to the appropriate utility immediately.

 FORMCHECKBOX 

All exposed cables should be given suitable protection against damage and those more than 1 m long should be supported by slings or props.

 FORMCHECKBOX 

Care must be taken near sewers and sewage pipes, since damaging them carries a double risk; toxic or flammable gases may be present in a foul sewer, from which there is also risk of infection from contact with the materials flowing.


	

	Additional controls considered necessary and further information:

 FORMCHECKBOX 

Location:  The position of any services in or near the proposed work area should be pinpointed as accurately as possible by means of a locating device, in conjunction with information already obtained. Various locators are available, the main types of locator are:-


 FORMCHECKBOX 

For further guidance on buried electricity cables refer to HSE Guidance Note HS (G) 47

 FORMCHECKBOX 

Refer to CITB Construction Site Safety


Method statement

 FORMCHECKBOX 
Yes  FORMCHECKBOX 
No

Permit to work
 FORMCHECKBOX 
Yes  FORMCHECKBOX 
No

COSHH Assessment

 FORMCHECKBOX 
Yes  FORMCHECKBOX 
No

PPE

 FORMCHECKBOX 
Yes  FORMCHECKBOX 
No

	Completed by: AM Holland
	Date: 17/11/21
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CJ Construction (Wales) Ltd

