Birds & Bats

A bat box such as a Schwegler 1WQ or suitable equivalent could be mounted on the south gable of the house
 
Wooden (or woodcrete) nest box with 3 sub-divisions to support 3 nesting pairs. To be placed under the eaves of buildings.

Entrance holes: 32mm diameter
Dimensions: H310 x W370 x D185mm
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Figure 1 - Rear Elevation
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Figure 2 - Side elevation
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Fig 2 Woodcrete house sparrow external nesting box
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Fig 1 Schwegler 1WQ bat box




