


Construction Noise Management Plan 

1.1 	Objective 

This management plan defines the measures to control and limit noise emissions and vibration levels, at residential properties and Dan Y Bryn Residential Home in the vicinity of the Project. 

1.1.1 	General Requirements – Noise 

Best Practicable Means (BPM) of noise control will be applied during construction works to minimise noise (including vibration) at neighbouring residential properties and other sensitive receptors arising from construction activities. 
The general principles of noise management are given below: 

Control at source:
 
· Equipment – noise emissions limits for equipment brought to site. 
· Equipment – method of directly controlling noise e.g. by ensuring plant and machinery is functioning according to the manufacturers specifications. 
· Equipment - indirect method of controlling excessive and prolonged noise e.g. acoustic screens. 

Control across site by: 

· Administrative and legislative control, 
· Control of working hours, 
· Control of delivery areas and times, 
· Careful choice of compound location, 
· Noise Monitoring, to check compliance with noise level limits, 
· Many of the activities which generate noise can be mitigated to some degree by careful operation of machinery and use of tools. This can be addressed by tool box talks and site inductions.

 
1.2 	Best Practicable Means 

BPM are defined in Section 72 of the Control of Pollution Act 1974 and Section 79 of the Environmental Protection Act 1990 as those measures which are:  
“reasonably practicable having regard among other things to local conditions and circumstances, to the current state of technical knowledge and to financial implications”. 

The Environment Agency require its contractors to consider mitigation in the following order:
 
· BPM as identified above, including: 

· Noise and vibration control at source: for example the selection of quiet and low vibration equipment, review of construction methodology to consider quieter methods, location of equipment on site, control of working hours, the provision of acoustic enclosures. 
· Screening: for example local screening of equipment; 
· Construction working hours should be carefully managed. All works should take place between normal working hours 08:00 and 16:30, Monday to Friday; 08:00 and 13.00 Saturday.
· 
The recommendations of BS5228: 2009+A1:2014 ‘Code of practice for Noise and Vibration Control on Construction and Open Sites’, will be implemented, together with the specific requirements of this management plan. 

1.3 	Consultation 

The maintenance of good community relations is vital. Experience shows that construction noise has the potential to cause disturbance but can be tolerated if prior warning and explanation has been given to residents. In particular advice regarding the nature of construction works, the duration of the works and mitigation measures to be implemented can help to reduce people’s reaction to noise. Contractors will consult local residents/communities regarding works and to give them details of a responsible appointed person on site who will be able to deal with queries.

1) Occupiers of adjacent properties will be informed by the Contractor of the works taking place, including the duration and likely noise and vibration effects. In the case of work required in response to an emergency, the Environment Agency and local residents will be advised as soon as reasonably practicable that emergency work is taking place. Potentially affected residents will also be notified of the helpline number for the contractor.  
 
2) A scheme of noise and vibration monitoring will be undertaken and assessed periodically during construction. Monitoring would aim to demonstrate that noise levels are being sufficiently controlled in order to protect residents from adverse noise and vibration levels. 


 
1.4 	Noise and Vibration Control Measures 

· Vehicles and mechanical plant will be maintained in a good and effective working order and operated in a manner to minimise noise emissions. The contractor will ensure that all plant complies with the relevant statutory requirements; 
· Compressor, generator and engine compartment doors will be kept closed and plant turned off when not in use; 
· All pneumatic tools will be fitted with silencers/mufflers; 
· Care would be taken when unloading vehicles to avoid un-necessary noise; 
· Restrict the number of plant items in use at any one time; 
· Reduce the speed of vehicle movements; 
· Ensure that operations are designed to be undertaken with any directional noise emissions pointing away from noise-sensitive receptors; 
· When replacing older plant, the quietest plant available will be considered; 
· Drop heights will be minimised when loading vehicles with rubble; 
· Vehicles will be prohibited from waiting within the site with their engines running or alternatively, located in waiting areas away from sensitive receptors; 
· Temporary noise screens will be used to reduce noise from particularly noisy activities and   
· Hours of operation will be strictly adhered to and any deviations will be with the consent of the local authority. 

2.1.5 	Construction Traffic
 
The Contractor will incorporate the following measures into the scheme to avoid noise related impacts from construction traffic: 
 
· Vehicles will not wait or queue up with engines running on the site or the public highway; 
· Vehicles will be properly maintained to comply with noise emissions standards; 
· Deliveries will be restricted to be within working hours of the site; and 
· Design and routing of access routes will minimise vehicle noise and the need to perform reversing manoeuvres. 

3 Summary 
This reports gives details of a noise construction management plan to be implemented by the appointed contractor prior to and during the construction of the Project. 
Best Practicable Means (BPM) of noise control are outlined and will be applied by the contractor during construction works to minimise noise (including vibration) at neighbouring residential properties and other sensitive receptors arising from construction activities. 
Specific mitigation measures will be implemented by the contractor during those construction activities identified as having the highest potential to cause disturbance from either noise and or vibration. 
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