

Finished lighting plan and Temp Construction Lighting plan.
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Description automatically generated]

The above lighting plan for the finished dwelling shows two low output down lights either side of each pedestrian entrance into the property. The lights will not be directed onto vegatation and will be a permenant fixture to the house once completed. Consideration has been given to the retention of Dark corridors and the minimul lighting required for occupoants safety when entering and exiting the dwelling has been proposed. 
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Description automatically generated]

The temporary construction lighting consists of 1.5w low output down lights. These lights are fitted at the pedestrian entrances to the temporary accommodation during the building phase. They are no directed at any vegetation. The timescale for the construction will be a proposed start build date of January 2023 with a proposed finished construction date of May 2024. During this time these will be the only lights on site. Once the construction phase has been completed the static caravan and touring caravans will be removed allowing for the construction of the driveway. The temporary lighting will be removed at the same time. 
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