
1. Environmental Issues

We will follow best practice for controlling environmental issues on site.

1.1. Site Set Up
1.1.1. Deliveries will be made to a materials and stores area established on the site furthest from the nearby stream, the Red Jacket Pill.
1.1.2. A one way system will be established for all site vehicles.
1.1.3. Fuel storage and COSHH storage areas will be established within the stores area.
1.1.3.1. Spill kits will be available at these locations.
1.1.4. A 10mph speed limit will be posted and enforced on site.
1.1.5. “Enviropad” spill mats will be used instead of drip trays to remove the problem of polluted ponding water sitting in drip trays.
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6.2. Site Drainage
6.2.1. A vegetation corridor will be left between the site and the river to act as a buffer to prevent silt entering the stream.
6.2.2. Cut off ditches will be established around the perimeter of the construction site to intercept run-off.
6.2.3. Water from excavations will be pumped through silt bags into grassy areas well away from the river. As evidenced from the trial holes excavated during The S.I. the subsoil strata is highly permeable, and as the majority of excavations are less than 1.0m deep little or no ground water is anticipated.  However the installation of the Interceptor close to the small building at the South end of the site will require a 3.0m deep excavation which will involve a dirty water pump discharging via a silt bag into the stilling pond located as shown on the plan. After allowing for further settlement the water will be discharged onto the permeable surface and allowed to percolate away.
6.2.4. Plant and wheel washing will be carried out in a designated area at least 10m from the river. At the location shown on the plan an existing dedicated concrete slab is present with a central sump which collects all washings and sediment from washing operations.  A submersible pump will be set in the gully transferring the wash water into an IPC which will be transported to treatment off – site.
6.2.4.1. Run-off will be collected in a small settlement pond.
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