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TAPCOSLATE CLASSIC

STOCKED

slate... but not as you know it!

Whether you have a conservatory, modern house or a listed building, TapcoSlate Classic
adds splendour, elegance and tradition to your home. It is authentically shaped with

textured surfaces and riven edges moulded from authentic slates that make TapcoSlate
Classic almost indistinguishable from natural slate - yet it has an even more refined
appearance. TapcoSlate Classic will not crack, break or delaminate, and its product
formulation and manufacturing processes provide durability, performance, and longevity
for many years to come. By providing a lightweight and easily-installed product, installation

costs are lower, with less waste!

« Lightweight - a5 low as 12kg per square metre.

« Easyto install with pre-marked nailing and exposure guides and spacers

« Easiy cut with a fine-toothed saw or sharp utility blade.

« Builtin camber for tighter fit when fixed in situ

« No sorting clipping, or drilling prior to roof loading. Packaged in bundles of 25
for easy handling

« Fittings (ridges and hips) are mechanically fixed,

804 P EWTE R G R EY « Choice of colours (7 standard colours and one Mix stocked for immediate

availability)
* 40-year warranty.
« Fully tested to BBA, UKTA and ETA standards, and has UKCA and CE marking,

including fire rating, wind, driven snow &rain, and water absorption REQUEST A FREE SAMPLE

« BRE testing for wind-driven rain found Taposlate Classic to perform much

stronger than all equivalent materials tested and at a lower pitch.

« TapcoSlate Classic is not made from recycled plastics but is manufactured
801 STONE BLACK 809 RED ROCK 814 OLVE GREEN CONTAGIUS
from recyclable virgin limestone and polypropylene.
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