Drainage Statement – 1-3 Office Place Glyncorrwg
Planning Application ID 2325032800 
Site Details 
Proposed Development: Change of Use from Social Club to single dwelling on first floor with commercial ground floor.
Detached 2 storey property, with concrete path surrounding property and a grassed garden area surrounding the front and rear of the property. The garden is bounded by existing fencing around the perimeter of the land. There are trees x2 to the rear fence line garden area. Detached outbuilding to rear of the property. Application site located adjacent to the roadway with a pasture field to the rear and garages/storage areas with grassland to each side.
Two small car parks, one residential and one commercial to be accessed via existing drive. Drawing supplied separately. 
Surface Water Management
The surface water discharge method is that surface water runoff is infiltrated to ground using permeable surfacing.  Due to the nature of the site it is not feasible to collect runoff for use. The edge of the car park will be planted with vegetation, such as native hedgerows in order to provide additional vegetated strips of land that will intercept and slow the water flow and will also filter out sediment and other pollutants while providing additional infiltration opportunities.
Constructional detail sheet for car parks and drive 
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Source:
“Guidance on the permeable surfacing of front gardens” - jointly published by the Communities and Local Government and the Environment Agency.
Glossary:
Open graded aggregate or sub-base
A gravel that is made up of a limited range of stone sizes so that there are open voids between the individual stones. This allows water to flow freely through it. Typical materials are known as 4/20 and Type 3 sub-base. 
Permeable surface
Any surface that allows water to soak through it. The surface can be permeable or porous. The surface made of materials that that allow water to soak through eg porous concrete and asphalt, gravel or from impermeable materials laid with gaps between blocks. 
Sub-base
A layer of compacted gravel that spreads the load from wheels so that the soil below is not overstressed.
Soak away 
An underground chamber or gravel filled trench that collects
water from the driveway and allows it to soak into the
ground.
Type 1 sub-base
A gravel that is made up of a range of stone sizes including fine material that fills the voids between the larger stones. This makes it hard for water to pass through it quickly. It is similar to hard core but of better quality.
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