NEATH PORT TALBOT COUNTY BOROUGH COUNCIL

The Town and Country Planning (Development Management Procedure) 
(Wales) Order 2015 (as amended)

HEAD OF ENGINEERING & TRANSPORT

HIGHWAYS OBSERVATIONS


PLANNING APPLICATION NO:	2/3/26/0051/00
APPLICANT:		MR J CAMPS
LOCATION:	LAND ADJACENT TO, 27 HEOL TABOR, CWMAVON, NEATH PORT TALBOT, SA12 9PS
PROPOSAL:	FOUR-BEDROOM DETACHED DWELLING WITH PARKING AND ASSOCIATED WORKS


The Highway Authority, in responding to the above application, provides the following substantive response: 

	No comment
	☐

	No objection  (subject to any specified conditions below)
	☐

	Concerns have been identified (see below for how those concerns can be addressed by the applicant
	☒

	Objection – on the grounds set out below
	☐



MY HIGHWAYS OBSERVATIONS ON THIS PROPOSAL ARE AS FOLLOWS:-

I have the following highway safety observations in respect of the above proposal.

1. The minimum width of the drive shall be increased to meet 3.6m width at its narrowest point and prior to first use of the dwelling shall be surfaced in porous material, or provision must be made to direct run-off water from the hard surface, to a permeable porous area or surface within the curtilage of the dwelling to a maximum gradient of 1 in 9, with no surface water aloud to flow out onto the public highway an permanently maintained as such thereafter.

2. Drawing 875-007 shows the columns fronting the vehicular access to be over 2m and boundary walls to be 1.5m in height, therefore impeding driver visibility. Pedestrian vision splays of 2.4 metres by 2.4 metres (measured from back of footway) shall be provided and maintained each side of each access within which nothing over 600mm in height shall be erected or allowed to grow.

3. Drawing 875-007 shows the columns fronting the vehicular access to be over 2m and boundary walls to be 1.5m in height, therefore impeding driver visibility. A 25 x 25 Vehicular Visibility Spay should be demonstrated from the centre point of this access and 2.4m into the curtilage of the site (driver seated position). Structures falling within this splay, either side of vehicular access’ are not to exceed more than 1m in height in accordance with Manual for Streets Guidance.

4. Prior to the occupation of the dwelling the forecourt boundary shall be set back to make up footway construction, this is to tie into the existing footway width along with the carriageway fronting the development site (being resurfaced) as detailed on the submitted plan 1875-010 Rev A.   
The highway works shall be constructed to the specification of the highway authority and shall be retained open and free for public use thereafter.

5. No surface water from within the curtilage of the dwelling shall be allowed to flow out onto the public highway or be connected into the highway drainage system.

6. The three parking bays, inclusive of the garage, shown on drawings 875-010 Rev A and PL875-002 shall be retained for such use thereafter.


NOTES TO APPLICANT

1. In order to ensure the road works you are required to undertake are carried out to the satisfaction of the Local Planning Authority and subsequently adopted you are advised prior to commencing any work on these works to contact the Head of Engineering and Transport at The Quays, Brunel Way, Baglan Energy Park, Neath, SA11 2GG (Highway Development Control – Telephone No. 01639 686850 or e-mail SAB-HDC@npt.gov.uk) to agree the specification, enter an adoption agreement and arrange on site inspection of your works.

For the construction of the vehicle crossover and carriageway resurfacing works, you should contact the Highways and Engineering Manager of Neath Port Talbot County Borough Council at The Quays, Brunel Way, Baglan Energy Park, Neath, SA11 2GG (Tel No. 01639 686407).  You should contact the above prior to commencing any works within the highway in order to arrange the necessary indemnity, licence and specification for the works.
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SIGNED: …………………….……		DATE: 	18/02/2026		
pp HEAD OF ENGINEERING & TRANSPORT


HIGHWAYS REF: OBS260051.docx
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