NEATH PORT TALBOT COUNTY BOROUGH COUNCIL

The Town and Country Planning (Development Management Procedure) 
(Wales) Order 2015 (as amended)

HEAD OF ENGINEERING & TRANSPORT

DRAINAGE OBSERVATIONS


PLANNING APPLICATION NO:	2/3/26/0051/00RECON 04.03.26
APPLICANT:		MR J CAMPS
LOCATION:	LAND ADJACENT TO, 27 HEOL TABOR, CWMAVON, NEATH PORT TALBOT, SA12 9PS
PROPOSAL:	FOUR-BEDROOM DETACHED DWELLING WITH PARKING AND ASSOCIATED WORKS (REVISED FLOOD CONSEQUENCES ASSESSMENT, DRAINAGE STATEMENT AND GROUND INVESTIGATION DETAILS 4/3/26)


The Highway Authority, in responding to the above application, provides the following substantive response: 

	No comment
	☐

	No objection  (subject to any specified conditions below)
	☒

	Concerns have been identified (see below for how those concerns can be addressed by the applicant
	☐

	Objection – on the grounds set out below
	☐

	SAB (SAB approval is required)
	☒


MY DRAINAGE OBSERVATIONS ON THIS RECONSULTATION DATED 04/03/26 ARE AS FOLLOWS:-

1. Should any springs or ground water seepage be encountered the on site works in that area shall cease until a scheme for collection and disposal of the water has been submitted to and approved in writing by the Local Planning Authority. No ground water shall ever be dischareged into the proposed drainage scheme.

2. There must be no interference, alteration or diversion of any ditch, watercourse, stream or culvert crossing or bordering the site, without prior consultation and agreement with the Authority.

3. Unless otherwise agreed in writing by the Local Planning Authority, foul water and surface water discharges shall be drained separately from the site. 

4. No surface water or Land drainage run-off shall be allowed to connect, either directly or indirectly, to the public sewerage system unless otherwise approved in writing by the Local Planning Authority.

5. Adequate provision shall be made for the drainage of the site, to ensure that the drainage of any adjoining land is not interrupted or otherwise adversely effected by the development during the life time of construction.

6. As the proposal involves the construction of a new dwelling and introduces more than 100m² of additional impermeable area, the development will require SAB approval prior to commencement, in accordance with Schedule 3 of the Flood and Water Management Act 2010.
While the drainage statement provides outline intentions, the LLFA notes that the proposals will require clarification and full supporting detail as part of the SAB application. 
Further information will be required on:

· Feasibility of infiltration, including BRE365 infiltration testing.
· A full SuDS strategy with specific SuDS components and justification through the SuDS hierarchy.
· Runoff calculations, attenuation sizing and climate change allowances.
· Management of surface water flood risk and overland exceedance routing.
· Confirmation of proposed surfacing materials (e.g., porous paving vs tarmac) and associated design details.
· A scaled drainage layout, levels and construction details.
· A maintenance plan for all drainage / SuDS features.
· Integration of SuDS design with observations in the FCA regarding local overland flow routes.

These matters must be addressed through a separate formal SAB application.


NOTES TO APPLICANT






SIGNED: Miss A. Smith				DATE: 	25/03/2026		
pp HEAD OF ENGINEERING & TRANSPORT


DRAINAGE REF: DOBS260051-R04.03.26

