Armco Barrier 
Approximately 15 linear metres either side of the barrier/gate (30m in total). Galv coating. Height of the barrier will be between 700-800mm from the ground.
Typical example below.
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