NEATH PORT TALBOT COUNTY BOROUGH COUNCIL

The Town and Country Planning (Development Management Procedure) 
(Wales) Order 2015 (as amended)

HEAD OF ENGINEERING & TRANSPORT

DRAINAGE OBSERVATIONS


PLANNING APPLICATION NO:	2/3/20/0010/00
APPLICANT:		ABODE WATERSTONE LTD
LOCATION:	HERITAGE GATE, COED DARCY, NEATH
PROPOSAL:	DRAINAGE PROPOSALS


The Highway Authority, in responding to the above application, provides the following substantive response: 

	No comment
	☐
	No objection  (subject to any specified conditions below)
	☐
	Concerns have been identified (see below for how those concerns can be addressed by the applicant
	☒
	Objection – on the grounds set out below
	☐


MY DRAINAGE OBSERVATIONS ON THIS PROPOSAL ARE AS FOLLOWS:-

THE FOLLOWING DRAINAGE CONCERNS HAVE BEEN IDENTIFIED:

1. The surface water design does not correspond with the previously approved drainage layout. 
a. Surface water pipe line between S12 to  SB.01 shall have a pipe diameter of 450mm not 300mm, 
b. Surface water line SB.01 to SB.02 shall have a pipe diameter of 300mm
c. Surface water line SB.02 to SB.03 shall have a pipe size diameter of 150mm. 

2. The Aco channel proposal is not suitable, it is recommended that an alternative design in the form of gulley’s are implemented in this location. 

3. All gulley’s require individual leaders into the main surface water line, gulley leaders cannot connect into each other. 


NOTES TO APPLICANT
Only surface water drainage pipes located within the highway will be adopted by the local authority, this can be clarified further at the post planning stage if needed, however we will still allow roof and yard connection from individual plots as previously agreed. 
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SIGNED: …………………….……		DATE:         04/02/2020		
HEAD OF ENGINEERING & TRANSPORT
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