[image: ]Erect chapter 8 pedestrian barrier either side of parking bay, install GRP tactile ramp and tactile floor panels to crossing point.
[bookmark: _GoBack]Access to/from footpath on north side to be via existing drop curbs and newly installed tactile floor panel.
All crossing points will be clearly sign posted from both directions.
Crossing point to the west of the site will be via existing Pelican Crossing.
3.7mtr clear opening to be maintained
From front of bus to corner of hoardings
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