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1.0 BACKGROUND INFORMATION

	Activity
	Description, notes or more information

	Applicant Name
	Mr Robert Franks 

	Application reference number
	CML2114

	Name of activity
	Works to Slipway, Afan Boat Club

	Brief description of activity
	Removing a concrete pad, installing a concrete retaining wall and new pontoons to make 
the slipway wider and safer

	Location of activity 
	51°35'10.7"N 3°47'53.5"W
51°35'10.7"N 3°47'53.0"W
51°35'09.4"N 3°47'53.5"W
51°35'09.5"N 3°47'54.3"W

	Timings of activity
	The works period will run from (approx. dates) 26/04/2021 to 02/07/2021 – these dates will be subject to marine license approval

	Extent of activity
	1. Carry out a pre-excavation survey of the working area
2. Excavation will be done behind the current concrete ‘pad’ and all material will be re-located 
3-6m away on the embankment behind the concrete pad. These works will be done using a 
banksman for safety measures. Daily excavation checks will be carried out and no trench is 
to be left open overnight/weekend. Adequate access and egress to be used and maintained 
into the excavation area. 
3. Once this has been completed, the removed material will be checked and ensured that all 
material stays in place on the embankment 
4. Temporary shutters will be inserted in preparation for the new retaining wall
5. After this has been done safely, a retaining wall will be installed behind the current concrete 
pad to ensure the integrity and strength of the embankment is improved. This will be done 
using rapid set, Portland cement. 
6. All concrete to be lifted into place using a ready-mix lorry
7. Once the new retaining wall has been safely installed, and has ‘set’, the current concrete pad 
can be removed. This will be removed to the same depth level as the slipway. 
8. The slip level will then be re-concreted, again using rapid set, Portland cement. 
9. RSJ girders will then be installed, in order for the installation of the new pontoons
10. Once safely completed, the new pontoon area will be installed. After these works have been 
completed, the slipway will be a lot wider and safer, as the slipway will be able to 
accommodate 2 boats (currently only 1). 
11. After the works have all been completed, all equipment will be demobilised from site

	Use or release of chemicals?
	No chemicals are used or released as part of this activity





2.0 SCREENING
Screening criteria to exclude activities from scoping:
	Activity
	Description, notes or more information

	Fast-track or accelerated marine licence activity?
	No.

	Maintaining pumps at pumping stations – if you do it 
regularly, avoid low dissolved oxygen levels during 
maintenance and minimise silt movement when 
restarting the pumps?
	No.

	Removing blockages or obstacles like litter or debris 
within 10m of an existing structure to maintain flow?
	No.

	Replacing or removing existing pipes, cables or 
services crossing over a water body – but not 
including any new structure or supports, or new bed 
or bank reinforcement?
	No.

	over water’ replacement or repairs to, for example 
bridge, pier and jetty surfaces – if you minimise bank 
or bed disturbance>
	No.



As such, we feel this a low-risk activity and does not require a screening. 






3.0 SPECIFIC RISK INFORMATION
Section 1: Hydromorphology

Assessment of impacts on hydromorphology:
	If the activity:
	Yes
	No
	Hydromorphology risk issue(s)

	Could impact on the 
hydromorphology (for 
example morphology or 
tidal patterns) of a high 
status water body.
	
	x
	No.

The AFAN ESTUARY INCL DOCKS water body does not have a high status.

	Could significantly impact the hydromorphology of a 
water body at less than 
high status
	
	x
	No. 

	Is in a water body that is 
heavily modified for the 
same use as your 
activity
	
	x
	No.



Section 2: Biology
Assessment of impacts on habitats:
	If the footprint of the activity is:
	Yes
	No
	Biology habits risk issue(s)

	0.5km2
or larger
	
	x
	No.

	1% or more of the water 
body’s area
	
	x
	No.

	Within 500m of any higher 
sensitivity habitat
	
	x
	No.
The works footprint is not within 500m of higher sensitivity habits

	1% or more of any lower 
sensitivity habitat
	
	x
	No. 
The works footprint is not 1% or more of any lower sensitivity habitat



Fish:
Assessment of impacts of fish:
	If the activity:
	Yes
	No
	Biology fish risk issue(s)

	Is in an estuary and could 
affect fish in the estuary, 
outside the estuary but 
could delay or prevent fish 
entering it or could affect 
fish migrating through the 
estuary
	
	x
	No.
The works will not affect fish in the estuary

	Could prevent normal fish 
behaviour like movement, 
migration or spawning (for 
example creating a physical 
barrier, noise, chemical 
change or a change in depth 
or flow)
	
	x
	No.
The works will not prevent normal fish behaviour such as movement, migration or spawning 

	Could cause entrainment or 
impingement of fish
	
	x
	No.
The works will not cause entertainment or impingement of fish



Section 3: Water quality
	If the activity:
	Yes
	No
	Water quality risk issue(s)

	Could affect water clarity, 
temperature, salinity, 
oxygen levels, nutrients 
or microbial patterns
continuously for longer 
than a spring-neap tidal 
cycle (about 14 days)
	
	x
	No.
The works will not affect water clarity, temperature, oxygen levels, salinity or microbial patterns

	Is in a water body with a 
phytoplankton status of 
moderate, poor or bad
	
	x
	No.


	Is in a water body with a 
history of significant and 
persistent algal blooms 
or toxic algal blooms
	
	x
	No.



Section 4: WFD protected areas
	If the activity: 
	Yes
	No
	Protected areas risk issue(s)

	Within 2km of any WFD protected area
	
	x
	No.
The works are not within 2km areas of any WFD protected areas

	
	
	
	



Section 5: Invasive non-native species (INNS)

	If the activity could:
	Yes
	No
	INNS risk issue(s)

	Introduce or spread 
INNS
	
	x
	No.
The works will not introduce or spread INNS. 



4.0 SUMMARY
	Receptor
	Potential risk to receptor?
	Note the risk issue(s) for impact assessment

	Hydromorphology
	No. 
	N/A

	Biology: Habitats
	No. 
	N/A

	Biology: Fish
	No. 
	N/A

	Water quality
	No. 
	N/A

	Protected areas
	No. 
	N/A

	Invasive non-native species
	No. 
	N/A
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