Appendix 
Vehicle Access
The site in its current state has a suitable access road from point A to B 
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The site welfare facilities are located at point C , all traffic both construction public will enter the site location via park avenue (point A) , however , only construction traffic will be able to travel beyond point D, this section will be fenced & gated to prevent any unauthorised access.
All construction vehicle must not block the access road , to prevent this we will introduce a holding  area where vehicles can park/stop , but still  maintain access for other vehicles accessing the 2 other facilities as noted.
The holding area will be located on the existing hardstanding area, point E.
The existing tarmac carpark will be maintained and utilised for both construction works and members of the public.

Suitable fencing and signage will be installed so that all personnel are aware of the arrangements 
During the site induction all construction personnel will be made aware of these arrangements, also all suppliers. 
[bookmark: _GoBack]Access to residential home and library will be as currently via point F, when construction works are being carried out on the main access road, a designed/approved traffic management system will be introduced to control traffic flow.
The site team will liaise with all suppliers to plan deliveries not for them to coincide with peak traffic times such as school starting & finishing, and any peak times for both the care home and Library.
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