As discussed, please see the below table which sets out our response to the comments raised within your previous email relating to the following application (ref. P2021/0027):
 
‘Details pursuant to the discharge of conditions 7 (Construction Method Statement), 11 (A scheme of landscaping including for the area of open space located towards the east end of the application site), 15 (Replacement of soakaway detail), 16 (New highway soakaway detail) and 17 (Access road and Footways Phasing Programme) of planning permission P2011/0486 approved on 11th December 2019’
 
As set out within my email yesterday, I was hoping that you may be able to provide some clarity on the comments raised in relation to Condition 16 (Highway Soakaway), where reference has been made to a ‘supporting email’ – I have left this highlighted in the below table, and we can look to response to any further comments on this when received under a separate email.
 
	App Ref. P2021/0027

	Condition No.
	Issue
	LPA Position
	Response

	7
	CMS
	How do they intend maintaining access to existing nursing home during phase 1 works via a designed approved traffic management system that as yet has not been provided?
 
The Construction Phase Health and Safety Plan and the Risk Assessment Method Statement do not appear to take into consideration the site has contaminated soils (Arsenic and PAH above the generic assessment criteria for Residential with Gardens properties). Clear and detailed measures need to be provided on how construction workers, adjacent site users surface run-off etc will be managed. A Material Management Plan will also be needed for the reuse of site won soils. It is important that the Remediation Scheme for this site and the Site Investigation report are both used to input the health & safety decision making and any risk to construction workers is managed at the site through the provision of appropriate Personal Protective Equipment (PPE) and the adoption of safe working practices as outlined in the CIRIA document 132 - "A Guide for Safe Working on Contaminated Sites".
	Please see enclosed documents confirming access arrangements with the nursing home. As can be seen within the attached correspondence, there has been ongoing dialogue between Manning Construction and the nursing home, resulting in an agreement. The following document evidence this:
 
1. Nursing Home Email Correspondence;
 
The following documents were referenced within the above email correspondence:
 
1. Proposed Site Plan;
1. Appendix - Vehicle Access;
1. Letter to Residents;
1. Temporary Closure of Footpath MOANG2 Glynneath; and
1. Temporary Footpath Closure Order.
 
Please also see enclosed the updated Construction Phase Health and Safety Plan that considers the contaminated soil (this is the same version as that submitted on the 11th June). 
 
It is considered that a Materials Management Plan is not required in this instance. Please see the attached email correspondence to Muttakir Mohammed which sets out this reasoning in detail (dated 8th April).
 

	11
	Landscaping
	The proposed layout plan 10- 19-01 Rev B conflicts with the tree protection areas (presumably this is the root protection shown on this plan done by Whittington)

· Wildflower areas
Neither of the wildflower mixes are native to this area or suitable for the soils. We recommend that they are changed to Emorsgate mix EM1 or EM2. Details of how these areas will be managed are
required.

· Trees
Sorbus ainifolia ‘Red Bird’ is not suitable for the wet conditions in this area. We recommend it is changed to a native species such as Sorbus aucuparia.
 
	An updated landscape proposals plan (drawing no. 002 rev. A) prepared by Whittington Landscape Architecture, was submitted in February 2021 which addresses the concerns raised. This has been attached to this email for ease.
 

	15
	Replacement Soakaway
	The Condition says notwithstanding drg 10-19-01 Rev B the location should not be in the proposed highway which will be part of a section 38 adoption agreement.
	Please see attached ‘Section 278 General Arrangement’ (Drg no. 10741/S278_770 rev. 05) where it can be seen that the replacement soakaway is positioned over 5 m from the highway curtilage.

	16
	Highway Soakaway
	Please provide directly to me the information provided as per the supporting email attached. (the officer in highways/drainage is off today so not sure what this means)
 
	??

	17
	Road and Footways Phasing Programme
	No comment.
	No action.


 
I hope and trust that the above and attached satisfies the comments raised in relation to application ref. P2021/0027, however, if any additional information is required, or you would like to discuss this further, please don’t hesitate to get in touch.
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