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	Project title
	Pant Celydd

	Location
	Margam, Port Talbot
	Contract no.
	21/9

	Method statement title
	DCWW Asset Protection
	Reference
	PC/DCWW

	Description of work
	To ensure full protection of DCWW Assets during the construction of 25 units and external works.

	This method statement has been developed and must be read with the following risk assessments

	Risk assessment reference
	Title

	215 (PC)
	Excavations: Buried DCWW Assets

	Drawing 20979/04 Rev B
	ENGINEERING SITE PLAN - EXISTING DCWW ASSET PLAN

	
	

	Work commences on
	March 2022

	Areas to be worked in
	Associated areas are highlighted on the attached drawing (20979/04 Rev B - ENGINEERING SITE PLAN - EXISTING DCWW ASSET PLAN)

Specifically area along the frontage of the site (West) along the line of the 300 diameter DCWW water main.

	Duration of work (actual or estimated)
	 1 month

	Number of workers (actual or estimated)
	 4

	Personnel (include details of  all personnel involved in the task and any specific training, skills or qualifications required)

	Name
	Position
	Competence details

	Harry Saunders
	
	

	Phil Williams
	
	

	Nick Hughes
	
	

	Tom Williams
	
	

	Emergency arrangement details

	

Fire/evacuation
	
[image: ]
First aid
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Pollution/spill
	




Other

	
	
	
	

	Personal protective equipment (PPE)requirements
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Other
	

Other

	Head
(EN397)
	Foot
(BS EN345-1)
	Hi- vis vest
	Hand
(BS EN388)
	Eye
(EN166)
	Hearing
(EN352-1)
	Fall arrest
	
	

	x
	x
	x
	x
	
	
	
	
	

	Construction dust (Note: construction dust is harmful and can lead to fatal lung diseases such as silicosis)

	Will the work create dust or fumes?
	
	Yes
	x
	No

	Identify specific control measures to avoid or minimise dust or fumes
	N/A

	Identify respiratory protective equipment (RPE) that will be required if dust or fumes cannot be avoided
	N/A



		Hazardous materials

	Are hazardous materials to be used?
	N/A
	
	
	
	Are COSHH/DSEAR data sheets available?
	N/A
	
	
	

	
Attach or identify specific controls required from COSHH risk assessment
	

	Permit required (tick below)

	
	Permit to work (general)
	
	Permit to enter
(confined spaces)
	
	Permit to dig YES

	
	Hot-work permit
	
	Out of hours work permit
	
	Other

	Details of person issuing permit
	Site Manager – Lee Bamford

	Description of safe method of work

	CONTRACTOR TO PROTECT & SECTION OFF ALL AREAS IDENTIFIED AS BEING IN THE VICINITY/EASEMENT LOCATION THROUGHOUT THE PROJECT / ACROSS THE SITE

DCWW WATER MAIN TRACE HAS BEEN CARRIED OUT AND LOCATION MARKED. 

WORKS TO BE CARRIED OUT ALONG WATER MAIN EASEMENT LOCATION:

* CONCRETE REINFORCED CROSSOVER FOR SITE ACCESS/EGRESS AS NECESSARY IN ORDER TO PROTECT DCWW WATER MAIN.

* REDUCED DIG FOR PARKING BAYS 
REDUCED DIG TO 400mm MAX TO BE CARRIED OUT WITH LIGHT PLANT FOLLOWING GUIDELINES. 

* NEW SERVICES EXCAVATIONS 
EXCAVATIONS (APPROX. DIG IN ADDITION TO 400mm REDUCED DIG - 350mm WATER & 200mm GAS/ELECTRIC) TO BE HAND DUG 

[bookmark: _GoBack]

	Tools, plant and equipment

	Type
	Details of inspections/test certificates

	2.5t Excavator  
	Date of inspection – 18/10/21

	3t Dumper

	n/a

	Hand digging tools 

	Date of inspection – 18/10/21

	
	

	
	

	Briefing register

	A copy of this briefing register must be attached to the method statement, together with other relevant information
(such as the associated risk assessments, permits or COSHH assessments).



	Supervisor in charge of the work

	I confirm that I have read and understand the requirements of this method statement and associated risk assessments and have communicated them to operatives under my control and to those who may be affected by its requirements.

Note: it is important that you test the operatives’ understanding and assume they have read and understood the method statement and risk assessments.

	Name
	
	Position
	
	Signature
	
	Date
	

	Operatives/workforce carrying out the work

	I understand and will agree to adhere to the contents of this method statement and the associated risk assessments.
I have attended a site induction/briefing that explained the general site rules and necessary site specific arrangements.

	Name
	Position
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


If you have any doubt about information given or contained in this method statement – ask for clarification.


	Index to Risk Assessments

	Section 1
Working at height
101 – Work at Height
102 – Scaffolding: General access
103 – Scaffolding: Erection and dismantling
104 – Scaffold Towers
105 – Mobile elevating work platforms
106 – Trestles
107 – Ladders
108 – Stepladders
109 – Stilts
110 – Safety nets: Provision and use
111 – Safety decking
112 – Fall arrest mats
113 – Work-restraint system
114 – Fall arrest harnesses
115 – Fragile roofs
116 – Flat roofs
117 – Sloping roofs
118 – Holes or edges
Section 2
Operations
201 – Asbestos containing materials (ACM)
202 – Asbestos cement products
203 – Demolition
204 – Electricity
205 – Fluorescent light removal/disposal
206 – Glazing
207 – Grit blasting
208 – Exposure to Lead
209 – Exposure to Noise
210 – Refurbishment
211 – Road works
212 – Welding
213 – Manual handling
214 – Excavations: General
215 – Excavations: Buried services
216 – Confined spaces – including manholes
217 – Work over/adjacent to water
218 – Falsework
219 – Erection of steel/timber structures
220 – Exposure to Discarded Needles and Syringes

	Section 3
Plant and lifting equipment
301 – Bitumen boilers and cauldrons
302 – Crane operations
303 – Scaffold crane
304 – Dumpers
305 – Excavators
306 – Forklift trucks and Telescopic Handlers
307 – Gin wheel
308 – Goods hoist
309 – Passenger hoist
310 – Maintenance of plant
311 – Piling operations
312 – Traffic management
313 – Driving of Motor Vehicles on Company Business
Section 4
Power tools
401 – Abrasive wheels
402 – Chainsaws
403 – Cartridge operated tools
404 – Portable power tools
405 – Woodworking machinery
406 – Vibration in hand-held power tools
407 – Stone-working machinery
408 – Nailing tool – Pneumatic/Gas
Section 5
Fire hazards
501 – Fire prevention
502 – Hot work
503 – Diesel fuel
504 – Highly flammable products
505 – Liquefied petroleum gas
Section 6
Special groups
601 – Unauthorised visitors
602 – Authorised visitors
603 – Authorised visitors - house purchasers
604 – Employment of young persons (under 18)
605 – Lone workers
Section 7
Miscellaneous
701 – Blank assessment
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