Additional Notes

The proposed work will be completed with materials and methods that will match the existing building as closely as possible, such as.
· Double roman roof tiles with matching dry verge system
· Brick and timber outer construction.
· Gold oak front door and rainwater goods.

Upon completion of the works, the existing front door will be removed to create an open plan entrance hall. The new front door will be 1000mm wide and incorporate a low threshold to accommodate wheelchair access. 



