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ROAD SAFETY AUDIT RESPONSE 
1. Project Details:
	[bookmark: _Hlk528749904]Report title:
	174 New Road, Skewen 

	Date:
	19/01/22

	Document reference and revision:
	RDW-DC-21-3557-RSA1

	Prepared by:
	Asbri Transport  

	On behalf of:
	Emerge Advertising 



2. Authorisation Sheet:
	Project:
	T21.171 - 174 New Road, Skewen

	Report title:
	Stage 1 Road Safety Audit 

	Prepared by:
	

	Name:
	Wyn Davies 

	Position:
	Principal Transport Planner 

	Signed:
	[image: ]

	Organisation
	Asbri Transport 

	Date: 
	19/01/22

	Approved by:
	

	Name:
	Patrick O’Connor 

	Position:
	Director 

	Signed:
	[image: ]

	Organisation
	Asbri Transport 

	Date: 
	19/01/22



3. Introduction:

It is proposed to replace the current static sign at 174 New Road (A4230) Skewen Neath with a digital LED 48 sheet billboard. 

The highway proposals include “erection of electronic advertisement board on gable end of property fronting onto New Road. The proposed site is situated along the southern side of the carriageway of New Road Skewen….It forms the main high street through Skewen”. 

[bookmark: _Hlk528750776]A stage 1 RSA was carried out on 12/11/22 by Safety Forum Limited, to audit the location, positioning and visibility of the screen.


4. Key Personnel
	Overseeing Organisation:
	Neath Port Talbot Highways 

	RSA Team:
	D Crawford, R Westhead  

	Design Organisation:
	Emerge Advertising, Asbri Transport Limited 





5. Road Safety Audit Decision Log:
	RSA Problem
	RSA recommendation 
	Design organisation response
	Overseeing Organisation Reponses 
	Agreed RSA action 

	3.1 Westbound vehicles passing in front of proposed advertising board may be difficult to see: Concern that Eastbound traffic may have difficulty seeing opposing traffic due to a bright display just above the headlights of opposing traffic. 
	Ensure that the mounting height of the advertising board is sufficiently separate from
westbound vehicles for eastbound drivers approaching on New Road.
	As well as being located to the side of the road the proposed sign will be 9 feet (2.7m) above the road and be unlikely to distract drivers.  
	Insert the Overseeing Organisation’s response
	Insert the design organisation’s and Overseeing Organisation’s agree action to the problem

	3.2 Uncertainty of display settings used: concern regarding potential for drivers to be distracted by bright and moving images.
	Ensure that the operation of the digital advertising board is in accordance with Guidance for Digital Roadside Advertising and Best Practice (2013, TfL, Waterman Transport & Development Limited), or other relevant best practice.
	The sign will be operating between 7am & 10pm, will not contain moving images, with brightness sensors fitted to adjust the brightness in relation to the prevailing ambient light.

Low illuminance panels will be equipped with pre-programmed  light levels operating below the recommended level (<300 cd/m²) with lower levels at night. The transition between adverts taking 2 seconds, the same as scrolling billboards so as not to distract drivers.

The sign will work on a rotation of 6 adverts with a dwell time of 10 seconds, which is double the recommended safety length stated in ILP - Lighting Guide.
	Insert the Overseeing Organisation’s response
	Insert the design organisation’s and Overseeing Organisation’s agree action to the problem



6. Design organisation and Overseeing Organisation statements:

The following statements should be signed by the design organisation and the Overseeing Organisation.

[bookmark: _Hlk528752199]Design organisation statement
	On behalf of the design organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the Overseeing Organisation.

	Name:
	

	Position:
	

	Signed:
	

	Organisation
	

	Date: 
	



Overseeing Organisation statement
	On behalf of the Overseeing Organisation I certify that:
1) the RSA actions identified in response to the road safety audit problems in this road safety audit have been discussed and agreed with the design organisation; and
2) the agreed RSA actions will be progressed. 

	Name:
	Insert name

	Position:
	Insert position

	Signed:
	Insert signature

	Organisation
	

	Date: 
	Insert date
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