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1.0 	Project Information 
1.1 Project Brief 
	37 Parish Road, Cwmgwrach.  


Project Title: 
 	 
	 
	37 Parich Road, Cwmgwrach, Neath. SA115SW.


Site Office Address: 
 	 
	01639 699509


Site Office Telephone: 
 	 
	craigmorgan241@tiscali.co.uk


Email: 
 	 
	The project is the development of a new build single detached four-bedroom home including integral garage. The property will be accessed via Parish Road in Cwmgwrach, Neath. Previously on the plot was a prefabricated bungalow. This has been removed and the site is bare ready for construction of the new dwelling. The new owners are residing on the site in a static caravan and will be on site during construction works. 
 


Project Description: 
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1.2 Relevant Planning Conditions 
This Construction Method Statement (CMS) has been specifically prepared to respond to decision notice P2022/0495.

Condition 5 : No development shall take place, including any works of demolition until a 
Construction Method Statement has been submitted to, and approved in writing by, 
the Local Planning Authority. The approved Statement shall be adhered to 
throughout the construction period. The Statement shall provide for: 
 i. the parking of vehicles of site operatives and visitors 
 ii. loading and unloading of plant and materials 
 iii. storage of plant and materials used in constructing the development 
[bookmark: _Hlk113446842] iv. the erection and maintenance of security hoarding including decorative displays 
and facilities for public viewing, where appropriate 
 v. wheel washing facilities 
 vi. measures to control the emission of dust and dirt during construction 
[bookmark: _Hlk113447115] vii. a scheme for recycling/disposing of waste resulting from demolition and 
construction works. 
 
 Reason: 
 In the interest of highway and pedestrian safety, the environment, and the amenity of 
residents, and to ensure accordance with Policies BE1 and TR2 of the adopted 
Neath Port Talbot Local Development Plan
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2.0 	Construction Method Statement  
2.1 Project specific arrangements 
The location of the site is adjacent to residential dwellings. The immediate public highway access road is shared with local residents. Parish Road in Cwmgwrach has no through road and the plot is situated at the end of the road near a turning area. Parish road is wide enough for vehicles to travel in either direction but has no pavement for pedestrian use. As such pedestrians use the road to walk and take refuge on the verge should vehicles pass. 
 
All construction traffic will use Parish Road and have the ability to turn on the site or at the end of Parish road in a turning area. Both locations are large enough for heavy goods vehicle turning. Any construction traffic will be pre planned and managed by the owner to ensure there are no congestion issues arising from vehicles accessing the site. 
 
All transport leaving site will be monitored and controlled as not to leave site unless in a clean state, a wheel control wash will be installed at periods of the project to assist with the control. This could be via the use of a hose pipe or pressure washer, all water and discharge will also be controlled as not to discharge on the public highway or sewer. 
 
There is not space to introduce a one way vehicle system with separate entry and exit gates, there is however space to set up holding areas for incoming vehicles on site.  The secure vehicle gates will be set back from the public highway to avoid backlog. Management of deliveries will be completed to ensure vehicles are not delivering at the same time to prevent congestion within Parish Road. 
When delivered to site materials and work equipment will be off loaded by Hiab and dependent on size, stored in a container and the compound adjacent to the building footprint it is needed for.  As the building progresses materials will moved and stored onto the building floor plates close the work areas as appropriate. Plan shows the designated container and compound.  
 
Construction workers vehicles will be instructed not to park on surrounding streets and park within the construction site area as designated on the plan. 
 
During construction site accommodation and welfare facilities position will be in the static caravan as designated on the plan.   
 
2.2 Vehicular access to site 
 
Deliveries vehicles to the work site will approach from Empire Avenue and onto Parish Road.  Delivery vehicles leaving site to all directions must follow the reverse and exit via Parish Road. 

Subcontractors and suppliers will have these directions written into their purchase orders.  
 
A gateman / Site owner will be present at all times when deliveries are expected to ensure directions are adhered. 

At no time will Site workers vehicles or delivery vehicles be parked on the public highway. This is to ensure  flow of traffic and safety for other road users and pedestrians.

2.3 The parking of vehicles of site operatives and visitors 
 
There is strictly no parking for vehicles on surrounding roads and streets.  All parking will be within the construction site compound as indicated on the site layout.    
 
This restriction will be written into subcontractor orders, clarified again during pre-start checks and reinforced during site safety and environmental inductions before contractors start their works on site. 
2.4 Loading and unloading of plant and materials. 
 
Plant and Materials will be unloaded either on site by hand or Hiab as appropriate. 

All materials will be unloaded in the designated area and moved to required locations. Please see attached plan for unloading areas. 
 

2.5 Storage of plant and materials used in construction and the development 
 
Areas for the storage of materials and plant will be available on site. 
 
An area has been allocated adjacent to the site office / static Caravan to hold vehicles on the site plan.  Containers and skips will be located nearby the work areas to limit movements  
 	 
Plant will be parked in a safe manner and de-mobilised during non-working hours and break times. 
 
2.6 Wheel washing facilities 
A ‘’wheel wash’’ arrangement will be provided when required, however, a gateman and/or labourer will wash the wheels of all vehicles using a pressure washer or other means before leaving site 
 
Water control measures will be carried out at the site to soak away the waste water and dirt that will be created during wheel washing.   
 
As much hard core as possible will be placed on the site compound to minimise the amount of dirt created and make it easier to clean site should any excess dirt be created during the construction process. 
 
 


 
2.7 Measures to control the emission of dust and dirt during construction   
  
Site inspections will be conducted for air quality and dust issues on site when activities with a high potential to produce dust are being Carried out and during prolonged dry or windy weather conditions. 
 
When reasonably practicable in dry windy conditions areas will be damped down regularly to prevent dust forming on site. 
 
Any sawing or drilling works will only take place if water suppression systems or dust extracts are in place. 
 
Flexible plastic sheeting will be used to surround work activities where appropriate. 
 
Any skips located on site will be in a position limiting dust and rubbish. Also covers / sheeting will be used to prevent dust and also any other materials escaping. 
 
Storage of plant, material and machinery will be located away from residential neighbours.
 
      2.8 Nuisance Prevention  
 
The following measures are to be implemented to reduce the nuisance to neighbours, and to ensure they      have an appropriate amount of involvement with the project: 
 
· Vehicle and plant movements within the construction site boundaries are proposed to be 07:00 to 18:00hrs Monday to Friday, and 08:00hrs to 13:00hrs on Saturday.  

· All plant and machinery will be switched off when not in use. 
 
· There will be no burning of materials on site. 
2.9  Materials management further information 
2.10.1 Materials Management 
The following materials management measures will be employed: 
 
Materials are to be stored in designated storage areas as agreed with the Site Management (Owner). 
· Materials are to be stored correctly so as to prevent damage and subsequent waste.    
· Plastic reusable pallets will be used on site if practicable and affordable for the job. 
· Materials will be managed to ensure offcuts are used within the building process if practicable. 
· Materials take back schemes will be utilised should there be over ordering of any products to avoid waste. 
· Materials to be pre-cut where possible to decrease the margin for error on site. - 	Pre-fabricated components to be procured where practical. 
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2.10  Street works and measures to protect the Bridleway 
 
There will be some works outside the site boundary associated with the development such as utility services e.g. Electricity, gas, water, foul drainage, broadband and telecoms.  If these are within the public highway and rights of way they will be planned and agreed with the highways dept prior to the works commencing and carried out by suitably qualified contractors.  Traffic management notices, signs, barriers will be required. 
  
 
[bookmark: _Hlk113448414] 2.11     Recycling/disposing of waste resulting from demolition and construction works.

		Prior to purchase, the previous owner has demolished and removed the old prefabricated building. This was    completed in compliance with regulations at that time and the site is now free of any building or previous building   material. As such no demolition will be required. 

In relation to any waste produced by the construction process this will be cleared daily by the owner and stored until removed from site using a trailer and / or skips. 
 
2.12 Remediation of contaminated land if discovered 
 During ground works, drainage and landscaping activities contractors will be instructed to remain vigilant and if contamination is found works will cease in the area discovered.  No further works in the work area will be carried out until a remediation scheme is put in place and agreed with NPT Planning Authority. 

[bookmark: _Hlk113448502]2.13 . The erection and maintenance of security hoarding including decorative displays 
and facilities for public viewing, where appropriate.

Prior to construction at the site Harras security fencing will be erected near the entrance of the site. This will be set back to allow for a holding area for any deliveries and parking for contractors vehicles. The Harras fencing will include covers to obstruct the view of the site during construction and a viewing area will be designated near the site office / static caravan for public viewing if required. 
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