NEATH PORT TALBOT COUNTY BOROUGH COUNCIL

The Town and Country Planning (Development Management Procedure) 
(Wales) Order 2015 (as amended)

HEAD OF ENGINEERING & TRANSPORT

DRAINAGE OBSERVATIONS


PLANNING APPLICATION NO:	2/3/25/0842/00
APPLICANT:		MS EMILY BYRNE
LOCATION:	1 HENFAES ROAD, TONNA, NEATH, SA11 3DX
PROPOSAL:	DEMOLITION OF EXISTING LISTED BUILDING ON SITE, INCLUDING THE OUTBUILDINGS AND ERECTION OF 8NO. DWELLINGS (6NO. MARKET AND 2NO AFFORDABLE), WITH ASSOCIATED HIGHWAY, LANDSCAPING, DRAINAGE AND INFRASTRUCTURE WORKS.


The Highway Authority, in responding to the above application, provides the following substantive response: 

	No comment
	☐

	No objection  (subject to any specified conditions below)
	☒

	Concerns have been identified (see below for how those concerns can be addressed by the applicant
	☐

	Objection – on the grounds set out below
	☐

	SAB (SAB approval is required)
	☒


MY DRAINAGE OBSERVATIONS ON THIS PROPOSAL ARE AS FOLLOWS:-

1. It is noted that we have received a SAB Pre-Application reference SP2025/0034. Prior to any works commencing on site Full SAB approval will be required. To commence work is a breach of SAB approval required under Paragraph 7 (1) Schedule 3 of the Flood and Water Management Act 2010 whereby legal action will be taken by the Authority under The Sustainable Drainage (Enforcement) (Wales) Order 2018. Guidance and applications can be found on https://www.npt.gov.uk/sab 

2. Should any springs or ground water seepage be encountered the on site works in that area shall cease until a scheme for collection and disposal of the water has been submitted to and approved in writing by the Local Planning Authority. No ground water shall ever be discharged into the proposed drainage scheme.

3. There must be no interference, alteration or diversion of any ditch, watercourse, stream or culvert crossing or bordering the site, without prior consultation and agreement with the Authority.

4. Unless otherwise agreed in writing by the Local Planning Authority, foul water and surface water discharges shall be drained separately from the site. 

5. No surface water or Land drainage run-off shall be allowed to connect, either directly or indirectly, to the public sewerage system unless otherwise approved in writing by the Local Planning Authority.

6. Adequate provision shall be made for the drainage of the site, to ensure that the drainage of any adjoining land is not interrupted or otherwise adversely effected by the development during the lifetime of construction.

DRAINAGE NOTE TO APPLICANT

Please note that from 7th January 2019, all new developments of more than 1 house, or where a construction area is of 100m2 or more, plus if the SAB authority believe that any redevelopment of land has significant surface water drainage implications. This will require sustainable drainage - built in accordance with mandatory standards for sustainable drainage published by Welsh Ministers - to manage on-site surface water. More information is available in Schedule 3 of the Flood & Water Management Act 2010. 

These systems must be approved by the Council’s Highway Development Control service acting in its SuDS Approving Body (SAB) role before construction work begins.  In this respect it is essential that a developer of any such project gain SAB approval of its surface water drainage alongside any relevant planning permission. You will not be allowed to start construction until both permissions have been approved.

If you have not done so already, and your development would not fall into any of the relevant exceptions, you are therefore strongly encouraged to request further advice from the SAB.  Involving the SAB Officers in pre-application discussions will allow for SuDS drainage matters (to ensure suitability of proposed SuDs design in line with national standards and adequate site layout) to be considered alongside the assessment of planning merits. There is an additional charge for this service. This can be as part of any agreed further pre-application submissions with the Planning Authority (recommended) or independently/ direct with the SAB.  You are advised, however, that failing to engage in joint pre-application discussions has the potential to lead to delays and, most notably, the potential need to obtain further planning permission should any agreed SuDS design not be compliant with any relevant planning permission. Further details are available at www.npt.gov.uk/sab 
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SIGNED: …………………….……		DATE: 	02/01/2026		
pp HEAD OF ENGINEERING & TRANSPORT
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